SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( M1_4180ZL
	Type ( Engine )
	WagonShape ( M1_4180ZL.s )
	Size  ( 3.006mm 3.728m 19.105m )
	CentreOfGravity ( 0m 1.7m 0m )
	Mass ( 35t )
	WheelRadius ( 0.4m )
	InertiaTensor ( Box (3.0m 3.7m 19.0m) )
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 2e7N/m 0  )
			Damping ( 0.2e7N/m/s 0 )
			Break ( 2e7N 0 )
			r0 ( 0.1 1e9 )
		)
		CouplingUniqueType( "RussianSubway" )
		CouplingHasRigidConnection ()
	)
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 2e7N/m 0  )
			Damping ( 0.2e7N/m/s 0 )
			Break ( 2e7N 0 )
			r0 ( 0.1 1e9 )
		)
		CouplingUniqueType( "RussianSubway" )
		CouplingHasRigidConnection ()
	)	
	Buffers (
		Spring (
			Stiffness ( 1e7N/m 0 )
			Damping ( 1e6N/m/s 0 )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 3cm )
	DerailRailForce ( 70kN )
	DerailBufferForce ( 40kN )
	NumWheels ( 4 )
	Friction (
		5N/m/s		1		1mph		1		1
		1.1N/rad/s		1		-1rad/s		1		1
	)
	AntiSlip ()

	BrakeEquipmentType( "EP_brake" )

	BrakeSystemType( "EP" )
	MaxBrakeForce( 60000N )

	EmergencyBrakeResMaxPressure( 50 )
	TripleValveRatio( 2.3 )
	MaxReleaseRate( 50 )
	MaxApplicationRate( 9 )
	MaxAuxilaryChargingRate( 4 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 4 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )
	EmergencyResVolumeMultiplier( 1.15 )
	BrakeAirPressureGainInResForOnePoundFromPipe( 0.25 )

	BrakeDistributorFullServicePressure( 0 )
	BrakeDistributorMaxAuxilaryResPressure( 50 )
	BrakeDistributorEmergencyResPressure( 50 )
	BrakeDistributorReleaseRate( 10 )
	BrakeDistributorApplicationRate( 15 )
	BrakeDistributorTrainPipeControlRatio( 2.03 )
	BrakeDistributorNormalFullReleasePressure( 70 )

	PassengerCapacity ( 115 )

	Lights	( 4
		Light	(
			comment( Red light outer right )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.7 1.4 -9.569 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
			
		Light	(
			comment( Red light outer left )
			Type( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.7 1.4 -9.569 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
						
		Light	(
			comment( Red light outer right )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.7 1.4 -9.569 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
			
		Light	(
			comment( Red light outer left )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.7 1.4 -9.569 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.75 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		)
	Sound ( "M1_4180eng.sms" )
	)
Engine ( M1_4180ZL
	Wagon ( M1_4180ZL )
	Type ( Electric )
	MaxPower ( 440kW )
	MaxForce ( 220kN )
	MaxContinuousForce ( 90kN )					
	MaxVelocity ( 130kmh )
	MaxCurrent ( 2350A )
	WheelRadius ( 0.425m )
	Sanding ( 1mph )
	NumWheels ( 4 ) 

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )

	EngineBrakesControllerDirectControlExponent( 2 )


	BrakesEngineControllers( "Train, Dynamic, Blended" )
	DoesBrakeCutPower( 1 )
	BrakeCutsPowerAtBrakeCylinderPressure( 50 )				

	AirBrakesAirCompressorPowerRating( 4 )
	AirBrakesMainMinResAirPressure( 30 )
	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 1 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.5 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )
	AirBrakesHasLowPressureTest ( 1 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 10 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	EngineBrakesControllerEmergencyApplicationRate( 10 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 10 )
	EngineBrakesControllerFullServicePressureDrop( 28 )

	TrainBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 10 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 90 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 10 )
	TrainBrakesControllerFullServicePressureDrop( 28 )

	DynamicBrakesMinUsableSpeed( 1 )
	DynamicBrakesMaximumEffectiveSpeed( 25 )
	DynamicBrakesMaximumForce( 110kn )
	DynamicBrakesResistorCurrentLimit ( 1600 )
	DynamicBrakesCutInSpeed( 1 )
	DynamicBrakesMaxAirBrakePressure ( 150 )
	DynamicBrakesFadingSpeed( 50 )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 150 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 8 )
	DynamicBrakeHasAutoBailOff( 0 )

	DoesHornTriggerBell( 0 )

    	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 1 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed( 0 )
		MonitoringDeviceResetOnResetButton( 1 )
    		)
		
	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 17 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 106 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		MonitoringDeviceDoesSuppressionReset( 0 )
		)
	
        EngineControllers (
            Throttle ( 0 1 0.25 0 
                NumNotches ( 5 
                	Notch ( 0       0 Dummy )
                	Notch ( 0.25    0 Dummy )
                	Notch ( 0.50    0 Dummy )
                	Notch ( 0.75    0 Dummy )
                	Notch ( 1.00    0 Dummy )
                )	
            )
            Brake_Train ( 0 1 0.1 0.7
                NumNotches ( 3
                    Notch( 0   0 TrainBrakesControllerReleaseStart )
                    Notch( 0.2 1 TrainBrakesControllerEPApplyStart )
                    Notch( 0.8 0 TrainBrakesControllerEmergencyStart )
                )
            )

            DirControl ( -1 0 1 1 )
            Combined_Control( 0 1 0.5 0.75 throttle train )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )
    Name ( "M1_4180ZL" )
    Description (
	"M1)"
    )
	EngineOperatingProcedures (
	"So setzen Sie den Zug in Bewegung\n"+
	"1. 	Der Stromabnehmer wurde bereits ausgefahren. (Sollte dies aus irgendeinem Grund noch nicht geschehen sein, drücken Sie die P-TASTE, um den Stromabnehmer auszufahren.)\n"+	
	"2.	Drücken Sie die D-TASTE, um den Hauptsteuerhebel in die Position Leerlauf zu stellen.\n"+
	"	Hinweis: Wenn sich der Hauptsteuerhebel in der Stellung Leerlauf befindet, leuchtet eine grünes Licht auf.\n"+
	"3.	Drücken Sie die W-TASTE, um den Richtungshebel auf  Vorwärts zu stellen.\n"+
	"	Hinweis: Der Richtungshebel kann nur bedient werden, wenn sich der Regler in der Stellung Leerlauf befindet.\n"+
	"4.	Drücken Sie die D-TASTE, um den Hauptsteuerhebel in die Reglerkerbe 1 zu stellen.\n"+
	"5.	Wenn Sie schneller fahren möchten, drücken Sie die D-TASTE, um den Hauptsteuerhebel in eine höhere Reglerkerbe zu bewegen.\n"+
	"So bremsen Sie den Zug ab\n"+
	"1.	Drücken Sie die A-TASTE, um den Regler nach unten zu bewegen.\n"+
	"2.	Setzen Sie die Bremsen ein, wenn Sie noch weiter abbremsen möchten.\n\n"+   
	"So bedienen Sie die Zugbremsen\n"+
	"1.	Drücken Sie die Ä-TASTE, um die Zugbremse zu ziehen.\n\n"+
	"So lösen Sie die Zugbremsen\n"+
	"1. Drücken Sie die Ö-TASTE, um die Zugbremsen zu lösen.\n\n"+
	"So lösen Sie die Notbremse aus\n"+
	"1.	Drücken Sie die A-TASTE, um den Hauptsteuerhebel zur höchsten Bremseinstellung zu bewegen.\n"+
	"	- oder -\n"+
	"2.	Drücken Sie die RÜCKTASTE.\n\n"+
	"So fahren Sie rückwärts\n"+
	"1.	Halten Sie den Zug vollständig an.\n"+ 
	"2.	Drücken Sie die S-TASTE, um den Richtungshebel in die Position Rückwärts zu stellen.\n"+
	"	Hinweis: Der Richtungshebel kann nur bedient werden, wenn sich der Regler in der Stellung Leerlauf befindet.\n"+
	"4.	Drücken Sie die Ö-TASTE, um die Bremsen zu lösen.\n"+
	"5.	Schieben Sie den Regler langsam nach vorne (D-TASTE).\n\n"+
	"So lassen Sie Fahrgäste ein- und aussteigen\n"+
	"1. Halten Sie an einem Bahnhof an.\n"+
	"2. Drücken Sie die EINGABETASTE.\n"+
	"3. Warten Sie auf das 'Signal zur Abfahrt'.\n"+
	"TIPP: Verwenden Sie die Lokführerinformation 'Nächster Halt' (F10), um das Ein- und Aussteigen zu überwachen."
	)
)
