'             _______________________________________
'   ________|                                       |___________
'  \        |    Scania Citywide LFA BioEthanol     |          /
'   \	    |		Power curve and		    |         /
'    \      |           Fuel comsuption             |        /
'     \     |    Wizard © 2015, Edit: Ratti 2016    |       /
'     /     |_______________________________________|       \
'    /___________)                               (___________\



[const]
engine_J
3.35

[const]
engine_speedcontrol
1

[newcurve]
max_speed

[pnt]
0
0.7

[pnt]
10
1.0

[pnt]
86
1

[pnt]
88
0.7

[pnt]
90
0

[newcurve]
max_speed_ECAS

[pnt]
8
1

[pnt]
10
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
600

[const]
engine_governed_max_RPM
2450

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350


[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4


[const]
engine_starterM
1000

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
600
700

[pnt]
700
850

[pnt]
800
1100

[pnt]
1000
1450

[pnt]
1050
1600

[pnt]
1200
1600

[pnt]
1300
1600

[pnt]
1400
1530

[pnt]
1500
1450

[pnt]
1550
1350

[pnt]
1800
1250

[pnt]
1900
1175

[pnt]
2000
1150

[pnt]
2230
1100

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
475
300

[pnt]
600
0

[pnt]
700
-100

[pnt]
1000
-200

[pnt]
2200
-300

[newcurve]
engine_M_minThrottle_HighRPM

[pnt]
50
0

[pnt]
700
300

[pnt]
800
0

[pnt]
900
-100

[pnt]
1200
-200

[pnt]
2200
-300

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.8

[pnt]
1200
0.9

[pnt]
1800
0.8

[pnt]
2300
0.5

[newcurve]
engine_efficiency_throttle

[pnt]
0
0.2

[pnt]
0.4
0.4

[pnt]
0.6
0.5

[pnt]
0.8
0.75

[pnt]
1
1.0

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
240



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
88

[const]
kuehlerthermostat_opn
83

[const]
kuehlerthermostat_cls
80

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
0.35

[const]
engine_Qrate_cooling_factor
1000

[const]
engine_Qrate_fan_factor
0.7

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
2

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000


[newcurve]
engine_turbo_RPM_factor

[pnt]
0
0

[pnt]
600
0.5

[pnt]
1000
0.87

[pnt]
1550
0.9

[pnt]
2000
1.0


[newcurve]
engine_turbo_throttle_factor

[pnt]
0
0.2

[pnt]
0.6
0.7

[pnt]
1
1

[newcurve]
engine_turbo_boost

[pnt]
0
1

[pnt]
70
1

[pnt]
90
1.35

[pnt]
100
1.5

	g/kWh
[newcurve]
engine_fuel_consumption_map

[pnt]
0
0

[pnt]
1200
195

[pnt]
1370
192

[pnt]
1500
194

[pnt]
1700
194

[pnt]
1900
200

[pnt]
2100
211