[newcurve]
door2_xposition 

[pnt]
0
0
[pnt]
0.1
1
[pnt]
1
1

Door2 Ypoition

[newcurve]
door2_yposition

[pnt]
0
0
[pnt]
0.1
0.08
[pnt]
1
1

Door3 Xpoition

[newcurve]
door3_xposition

[pnt]
0
0
[pnt]
0.1
1
[pnt]
1
1

Door3 Ypoition
[newcurve]
door3_yposition
[pnt]
0
0
[pnt]
0.1
0.08
[pnt]
1
1


	Front/Back Door Acceleration (100%/s?

[const]
fdoor_acc
1.5

[const]
bdoor_acc
2.5

	Door Acceleration Variation (100%/s?

[const]
door_acc_var
0.0

	Front/Back Door Max Speed (100%/s)

[const]
fdoor_maxspeed
0.5

[const]
bdoor_maxspeed
1.5

[const]
door_maxspeed_var
0

	Front/Back Door Damper (100%/s)

[const]
door0_damper
6

[const]
door1_damper
6

[const]
door2_damper
2

[const]
door3_damper
12


		Dämpferkennlinie über Öffnungzustand:

[newcurve]
damper_f_close

[pnt]
0.2
1

[pnt]
0.8
0

[newcurve]
damper_f_open

[pnt]
0.2
0

[pnt]
0.8
0.8

[newcurve]
damper_b_close

[pnt]
0.2
1

[pnt]
0.8
0

[newcurve]
damper_b_open

[pnt]
0.2
0

[pnt]
0.8
0.6


	Door Stop Reflexion Coefficient

[const]
door_refl
0

	Automatic Back Door Time

[const]
doorAftOpenTime
3

	Busstop Brake will only be activated belov MaxKMH:

[const]
Door_Bremse_Halte_MaxKMH
2

'Vordertürflügel sind kombiniert und Hintertür manuell:

[const]
door_ManBackDoorFrontDoorCombined
1

'Sicherheits-Rebelüftung:

[const]
door_safe_reactivating
0

[const]
door_stop_request_killed_by_front_door
1

[const]
door_druckluft
1

[const]
door_needs_stopbrake
0

[const]
door_needs_stopbrakeswitch
0


[const]
electric_doors
1

[const]
thinking_doors
0

[const]
door_blocking
1

[const]
door_blocking_area
0.1

[const]
door_blocking_diff
0.03

[const]
door_blocking_speed
0.01





[newcurve]
door_0_opn_speed

[pnt]
0
0.5

[pnt]
0.4
0.5

[pnt]
0.5
0.3

[pnt]
0.55
0.5

[pnt]
0.8
0.5

[pnt]
0.975
0.04

[pnt]
1
0.15

[newcurve]
door_0_cls_speed

[pnt]
0
0.2

[pnt]
0.05
0.05

[pnt]
0.2
0.7

[pnt]
0.45
0.7

[pnt]
0.5
0.01

[pnt]
0.6
0.7

[pnt]
0.85
0.7

[pnt]
0.995
0.01

[pnt]
1
1

[newcurve]
door_1_opn_speed

[pnt]
0
0.7

[pnt]
0.4
0.7

[pnt]
0.5
0.4

[pnt]
0.55
0.7

[pnt]
0.8
0.7

[pnt]
0.975
0.05

[pnt]
1
0.2

[newcurve]
door_1_cls_speed

[pnt]
0
0.2

[pnt]
0.05
0.05

[pnt]
0.2
0.7

[pnt]
0.45
0.7

[pnt]
0.5
0.01

[pnt]
0.6
0.7

[pnt]
0.85
0.7

[pnt]
0.995
0.01

[pnt]
1
1

[newcurve]
door_2_opn_speed

[pnt]
0
1

[newcurve]
door_2_cls_speed

[pnt]
0
1

[newcurve]
door_3_opn_speed

[pnt]
0
1

[newcurve]
door_3_cls_speed

[pnt]
0
1

=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Türflügelstromverbrauch: 500W/Geschwindigkeit 1 (0.87 1/Ohm)

[const]
door_Rinv
0

.............................

=============================================
Malfunction-Parameter

[const]
door_malf_autobdoor_livetime_cyc
1000


