'##############
'Door Script
'##############

'Controls Doors

'(c) 2007-2009 Rüdiger Hülsmann
'(c) 2007-2009 Marcel Kuhnt

'Script Version: 1.3
'Omsi release: 2.0

'Needs:
'- elec

'Revision History:
'- Marcel Kuhnt		13.06.2009	Batterietrennschalter => elec_busbar_main
'- Marcel Kuhnt		21.06.2009	AI-Unterstützung hinzugefügt	
'- Rüdiger Hülsmann	24.10.2009	Ansteuerung des Kinderwagenwunsches modifiziert
'- Rüdiger Hülsmann	19.12.2009	Timer für Ausstiegstür jetzt Timegap-basiert, Bugfix: Tür schließt jetzt nur bei elec_busbar=1
'- RÜdiger Hülsmann	22.09.2010	Door light trigger value set to 0.1
'- RÜdiger Hülsmann	07.11.2010	Door speed based on reservoir pressure, air-operated doors made an option
'- Marcel Kuhnt		08.11.2010	AI procedure closing doors debugged
'- Rüdiger Hülsmann	21.11.2010	Front doors only operable when busbar on
'- Rüdiger Hülsmann	23.12.2010	External front door operation included, option: doors only operable with actual stop brake
'- Rüdiger Hülsmann	31.12.2010	Electric door function debugged
'- Rüdiger Hülsmann	05.01.2011	20h-switch
'- Rüdiger Hülsmann	07.01.2011	Backdoor manual switch sound debugged, 20h switch depending on bus type
'- Rüdiger Hülsmann	19.01.2011	Electric door support
'- Rüdiger Hülsmann	19.01.2011	Electric door support
'- Morozov Maxim	----------	Removed automatical back door. Added ramp animation... etc...
'- Alexey Vasiliev	09.03.2012	Added more doors for Citaro "Private Edition"
'- Sergey Wizard	14.11.2013	Added automatical back doors. Rework dooraft for citaro 3door
'- Alexey Vasiliev	13.12.2013	Added 4 door for Citaro G
'- Sergey Wizard	17.12.2013	Bugfix for dooraft (Citaro and Citaro G)
'--------------------------------------------------------------------------------



{trigger:bus_doorfront0}
	(L.L.elec_busbar_main) (L.L.bremse_halte_sw)  ! && &&
	(L.L.elec_busbar_main) (L.L.bremse_halte)  && && ||
	{if}
		(M.L.trg_bus_doorfront0)
	{endif}
	1 (S.L.cockpit_tuertaster1)
{end}

{trigger:bus_doorfront0_off}
	0 (S.L.cockpit_tuertaster1)
{end}

{trigger:bus_doorfront1}
	(L.L.elec_busbar_main) (L.L.bremse_halte_sw)  ! && &&
	(L.L.elec_busbar_main) (L.L.bremse_halte)  && && ||
	(L.L.door_20h_sw) ! &&
	{if}
		0 (S.L.door_kinderwagenwunsch)
		(M.L.trg_bus_doorback23)
	{endif}
	1 (S.L.cockpit_tuertaster2) (S.L.PAX_Exit0_Req)
{end}

{trigger:bus_doorfront1_off}
	0 (S.L.cockpit_tuertaster2) (S.L.PAX_Exit0_Req)
{end}

{trigger:bus_doorfront2}
	(L.L.elec_busbar_main) (L.L.bremse_halte_sw)  ! && &&
	(L.L.elec_busbar_main) (L.L.bremse_halte)  && && ||
	(L.L.door_20h_sw) ! &&
	{if}
		0 (S.L.door_kinderwagenwunsch)
		(M.L.trg_bus_doorfront5)
	{endif}
	1 (S.L.cockpit_tuertaster3) (S.L.PAX_Exit2_Req)
{end}

{trigger:bus_doorfront2_off}
	0 (S.L.cockpit_tuertaster3) (S.L.PAX_Exit2_Req)
{end}

{trigger:bus_doorfront3}
	(L.L.elec_busbar_main) (L.L.bremse_halte_sw)  ! && &&
	(L.L.elec_busbar_main) (L.L.bremse_halte)  && && ||
	(L.L.door_20h_sw) ! &&
	{if}
		0 (S.L.door_kinderwagenwunsch)
		(M.L.trg_bus_doorfront6)
	{endif}
	1 (S.L.cockpit_tuertaster4) (S.L.PAX_Exit5_Req)
		
{end}

{trigger:bus_doorfront3_off}
	0 (S.L.cockpit_tuertaster4) (S.L.PAX_Exit5_Req)
{end}

{trigger:bus_dooraft}
	(M.L.trg_bus_dooraft)

{end}

{trigger:bus_20h-switch}
	(C.L.cockpit_has_20h_switch)
	{if}
		(M.L.trg_bus_20h-switch)
	{endif}
{end}


{trigger:int_haltewunsch}
	1 (S.L.haltewunsch)
{end}

{trigger:door_haltewunsch}
	1 (S.L.haltewunsch) (S.L.door_haltewunsch_knopfdruck)
{end}

{trigger:door_haltewunsch_off}
	0 (S.L.door_haltewunsch_knopfdruck)
{end}

{trigger:cp_schalter_kinderwagen}
	(L.L.door_handsteuerung) ! (S.L.door_handsteuerung)
	{if}
		0 (S.L.door_kinderwagenwunsch)
		(T.L.ev_kippschalter_ein)
	{else}
		(T.L.ev_kippschalter_aus)
	{endif}
		
{end}

{trigger:door_kinderwagenwunsch}
	(L.L.bremse_halte) (L.L.door_handsteuerung) ! &&
	{if}
		1 (S.L.door_kinderwagenwunsch)
	{endif}
{end}


{macro:Door_Init}
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.fdoor_acc) + (S.L.doorAcc_0)
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.fdoor_acc) + (S.L.doorAcc_1)
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.bdoor_acc) + (S.L.doorAcc_2)
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.bdoor_acc) + (S.L.doorAcc_3)	
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.bdoor_acc) + (S.L.doorAcc_4)
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.bdoor_acc) + (S.L.doorAcc_5)
	1000 random 500 / 1 - (C.L.door_acc_var) * (C.L.bdoor_acc) + (S.L.doorAcc_7)
	
	
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.fdoor_maxspeed) + (S.L.doorMaxSpeed_0_norm)
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.fdoor_maxspeed) + (S.L.doorMaxSpeed_1_norm)
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.bdoor_maxspeed) + (S.L.doorMaxSpeed_2_norm)
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.bdoor_maxspeed) + (S.L.doorMaxSpeed_3_norm)	
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.bdoor_maxspeed) + (S.L.doorMaxSpeed_4_norm)
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.bdoor_maxspeed) + (S.L.doorMaxSpeed_5_norm)	
	1000 random 500 / 1 - (C.L.door_maxspeed_var) * (C.L.bdoor_maxspeed) + (S.L.doorMaxSpeed_7_norm)
	
	(C.L.door_refl) (S.L.doorRefl_0)
	(C.L.door_refl) (S.L.doorRefl_1)
	(C.L.door_refl) (S.L.doorRefl_2)
	(C.L.door_refl) (S.L.doorRefl_3)
	(C.L.door_refl) (S.L.doorRefl_4)
	(C.L.door_refl) (S.L.doorRefl_5)
	(C.L.door_refl) (S.L.doorRefl_7)
	
{end}

{macro:Door_Frame}
	(M.L.Door0_Calc)
	(M.L.Door1_Calc)
	(M.L.DoorAftCalc)
	(M.L.Door2_Calc)
	(M.L.Door3_Calc)
	(M.L.Door4_Calc)
	(M.L.Door5_Calc)
	(M.L.Door7_Calc)

	(L.L.door_0) 0.9 > (S.L.PAX_Entry0_Open) (S.L.PAX_Entry1_Open)
	(L.L.door_3) 0.9 > (S.L.PAX_Exit0_Open) (S.L.PAX_Exit1_Open)
	(L.L.door_5) 0.9 > (S.L.PAX_Exit2_Open) (S.L.PAX_Exit3_Open)
	(L.L.door_7) 0.9 > (S.L.PAX_Exit4_Open) (S.L.PAX_Exit5_Open)



'	"Dauerfeuer"-Haltewunsch über Kinderwagenschalter (macht genau dasselbe wie der "trigger:int_haltewunsch"):
	(L.L.door_handsteuerung) (L.L.door_haltewunsch_knopfdruck) ||
	{if}
		1 (S.L.haltewunsch)
	{endif}

'	Setzen der Haltestellenbremse erst bei Stillstand des Busses:
	(L.L.bremse_halte_sw) (L.L.door_20h_sw) ||
	(L.L.bremse_halte) ! (L.L.Velocity) (C.L.Door_Bremse_Halte_MaxKMH) < && &&
	{if}
		(L.L.elec_busbar_main)
		{if}
			(T.L.ev_haltebremse_an)		
			1 (S.L.bremse_halte)
		{endif}
	{endif}
	
	(M.L.DoorAft_Open)

'	Türfreigabekriterium

	(L.L.bremse_halte_sw) (L.L.bremse_halte) && (S.L.door_freigabe)

'	Haltewunschlampe:
	(L.L.haltewunsch) (L.L.door_2) 0.2 < (L.L.elec_busbar_main) && &&
	{if}
		1 (S.L.haltewunschlampe)
	{else}
		0 (S.L.haltewunschlampe) (S.L.haltewunsch)
	{endif}

'	Abfall des Kinderwagenwunsch-Relais bei fehlender Stromversorgung:

	(L.L.elec_busbar_main) 0 = 
	{if}
		0 (S.L.door_kinderwagenwunsch)
	{endif}

'	Beleuchtung der Einstiege

	(L.L.elec_busbar_main)
	{if}
		(L.L.door_0) 0.1 > (L.L.door_1) 0.1 > || (S.L.door_light_1)
		(L.L.door_2) 0.1 > (L.L.door_3) 0.1 > || (S.L.door_light_2)
		(L.L.door_5) 0.1 > (S.L.door_light_3)
		(L.L.door_7) 0.1 > (S.L.door_light_4)
	{else}
		0 (S.L.door_light_1) (S.L.door_light_2) (S.L.door_light_3) (S.L.door_light_4)
	{endif}

'	Druckabhängige Türgeschwindigkeit
	
	(C.L.door_druckluft)
	{if}
		(L.L.doorMaxSpeed_0_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_0)
		(L.L.doorMaxSpeed_1_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_1)
		(L.L.doorMaxSpeed_2_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_2)
		(L.L.doorMaxSpeed_3_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_3)		
		(L.L.doorMaxSpeed_4_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_4)
		(L.L.doorMaxSpeed_5_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_5)				
		(L.L.doorMaxSpeed_7_norm) (L.L.bremse_p_Tank04) 100000 - 850000 / (S.L.doorMaxSpeed_7)
	{endif}
'----------------------
'	AI-Ablauf:

(L.L.AI_Scheduled_AtStation) s0
1 =
{if}
'Wenn Türen geöffnet werden sollen:
	(L.L.Velocity) (C.L.Door_Bremse_Halte_MaxKMH) <
	{if}
'Nur, wenn v < maxkmh, sonst warten
'Taster jeweils nur betätigen, falls noch nicht an
		(L.L.bremse_halte_sw) !
		{if}
			(M.L.trg_bus_dooraft)
		{endif}
		(L.L.doorTarget_0) ! (L.L.door_AI_timer) 0.3 > &&
		{if}
			(M.L.trg_bus_doorfront0)
		{endif}
		(L.L.doorTarget_1) ! (L.L.door_AI_timer) 0.6 > &&
		{if}
			(M.L.trg_bus_doorfront1)
		{endif}
		(L.L.doorTarget_23) ! (L.L.door_AI_timer) 0.6 > (L.L.haltewunsch) && &&
		{if}
			(M.L.trg_bus_doorback23)
		{endif}
		(L.L.doorTarget_45) ! (L.L.door_AI_timer) 0.6 > (L.L.haltewunsch) && &&
		{if}
			(M.L.trg_bus_doorfront5)
		{endif}
		(L.L.doorTarget_67) ! (L.L.door_AI_timer) 0.6 > (L.L.haltewunsch) && &&
		{if}
			(M.L.trg_bus_doorfront6)
		{endif}
	{else}
		0 (S.L.door_AI_timer)
	{endif}
	(L.L.door_AI_timer) (L.S.Timegap) + (S.L.door_AI_timer)
{else}
l0 -1 =
{if}
'Wenn Türen geschlossen werden sollen:
'Taster jeweils nur betätigen, falls noch nicht aus:
	(L.L.doorTarget_1)
	{if}
		(M.L.trg_bus_doorfront1)
		0 (S.L.door_AI_timer)
	{endif}
	(L.L.doorTarget_0) (L.L.door_AI_timer) 0.3 > &&
	{if}
		(M.L.trg_bus_doorfront0)
	{endif}
	(L.L.doorTarget_23) (L.L.door_AI_timer) 0.3 > &&
	{if}
		(M.L.trg_bus_doorback23)
	{endif}
	(L.L.doorTarget_45) (L.L.door_AI_timer) 0.3 > &&
	{if}
		(M.L.trg_bus_doorfront5)
	{endif}
	(L.L.doorTarget_67) (L.L.door_AI_timer) 0.3 > &&
	{if}
		(M.L.trg_bus_doorfront6)
	{endif}
'Haltestellenbremse erst wegnehmen, wenn alle Türen zu. Dann auch erst den Bus AI-mäßig freigeben:
	(L.L.door_0) 0.1 <
	(L.L.door_1) 0.1 < &&
	(L.L.door_2) 0.1 < &&	
	(L.L.door_4) 0.1 < &&
	(L.L.door_5) 0.1 < &&	
	(L.L.door_7) 0.1 < &&
	{if}
		(L.L.bremse_halte_sw) (L.L.door_AI_timer) 0.3 > &&
		{if}
			(M.L.trg_bus_dooraft)
		{endif}
		(L.L.bremse_halte_sw) !
		{if}
			0 (S.L.AI_Scheduled_AtStation)
		{endif}
	{else}
'Sollte eine der Türen auf sein und die Haltestellenbremse aus, dann sofort diese einlegen
		(L.L.bremse_halte_sw) !
		{if}
			(M.L.trg_bus_dooraft)
		{endif}
		(L.L.doorTarget_0) !
		(L.L.doorTarget_1) ! &&
		(L.L.doorTarget_23) ! &&
		(L.L.doorTarget_45) ! &&
		(L.L.doorTarget_67) ! &&
		{if}
			0 (S.L.door_AI_timer)
		{endif}
	{endif}
	(L.L.door_AI_timer) (L.S.Timegap) + (S.L.door_AI_timer)
{endif}
{endif}


{end}




{macro:Door0_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_0)
		{if}
			(L.L.door_0) (F.L.door_0_opn_speed) (S.L.doorMaxSpeed_0)
		{else}
			(L.L.door_0) (F.L.door_0_cls_speed) (S.L.doorMaxSpeed_0)
		{endif}

		(C.L.fdoor_acc) (S.L.doorAcc_0)

		(L.L.doorTarget_0) ! (L.L.doorSpeed_0) s0 abs 0.05 > (L.L.door_0) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_0) <
			{if}
				(L.L.doorSpeed_0) (L.L.doorAcc_0) (L.S.Timegap) * - (S.L.doorSpeed_0)
			{else}
				(L.L.doorSpeed_0) (L.L.doorAcc_0) (L.S.Timegap) * + (S.L.doorSpeed_0)
			{endif}
			(L.L.door_0) (L.L.doorSpeed_0) (L.S.Timegap) * + (S.L.door_0)
		{else}
			(L.L.doorSpeed_0) abs 0.05 > (L.L.door_0) 1 < || (L.L.doorTarget_0) &&
			{if}
				l0 (L.L.doorMaxSpeed_0) <
				{if}
					(L.L.doorSpeed_0) (L.L.doorAcc_0) (L.S.Timegap) * + (S.L.doorSpeed_0) 
				{else}
					(L.L.doorSpeed_0) (L.L.doorAcc_0) (L.S.Timegap) * - (S.L.doorSpeed_0) 
				{endif}
				(L.L.door_0) (L.L.doorSpeed_0) (L.S.Timegap) * + (S.L.door_0)
			{else}
				0 (S.L.doorSpeed_0)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_0) ! (L.L.doorSpeed_0) s0 abs 0.05 > (L.L.door_0) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_0) <
			{if}
				(L.L.doorSpeed_0) (L.L.doorAcc_0) (L.S.Timegap) * - (S.L.doorSpeed_0)
			{endif}
			(L.L.door_0) (L.L.doorSpeed_0) (L.S.Timegap) * + (S.L.door_0)
		{else}
			(L.L.doorSpeed_0) abs 0.05 > (L.L.door_0) 1 < || (L.L.doorTarget_0) &&
			{if}
				l0 (L.L.doorMaxSpeed_0) <
				{if}
					(L.L.doorSpeed_0) (L.L.doorAcc_0) (L.S.Timegap) * + (S.L.doorSpeed_0) 
				{endif}
				(L.L.door_0) (L.L.doorSpeed_0) (L.S.Timegap) * + (S.L.door_0)
			{else}
				0 (S.L.doorSpeed_0)
			{endif}
		{endif}
	{endif}

	(L.L.door_0) 1 >
	{if}
		(T.L.ev_doorhitopen_0)
		1 (S.L.door_0)
		(L.L.doorSpeed_0) /-/ (L.L.doorRefl_0) * (S.L.doorSpeed_0)
	{else}
		(L.L.door_0) 0 <
		{if}
			(T.L.ev_doorhitclose_0)
			0 (S.L.door_0)
			(L.L.doorSpeed_0) /-/ (L.L.doorRefl_0) * (S.L.doorSpeed_0)
		{endif}
	{endif}
{end}

{macro:Door1_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_1)
		{if}
			(L.L.door_1) (F.L.door_1_opn_speed) (S.L.doorMaxSpeed_1)
		{else}
			(L.L.door_1) (F.L.door_1_cls_speed) (S.L.doorMaxSpeed_1)
		{endif}

		(C.L.fdoor_acc) (S.L.doorAcc_1)

		(L.L.doorTarget_1) ! (L.L.doorSpeed_1) s0 abs 0.05 > (L.L.door_1) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_1) <
			{if}
				(L.L.doorSpeed_1) (L.L.doorAcc_1) (L.S.Timegap) * - (S.L.doorSpeed_1)
			{else}
				(L.L.doorSpeed_1) (L.L.doorAcc_1) (L.S.Timegap) * + (S.L.doorSpeed_1)
			{endif}
			(L.L.door_1) (L.L.doorSpeed_1) (L.S.Timegap) * + (S.L.door_1)
		{else}
			(L.L.doorSpeed_1) abs 0.05 > (L.L.door_1) 1 < || (L.L.doorTarget_1) &&
			{if}
				l0 (L.L.doorMaxSpeed_1) <
				{if}
					(L.L.doorSpeed_1) (L.L.doorAcc_1) (L.S.Timegap) * + (S.L.doorSpeed_1) 
				{else}
					(L.L.doorSpeed_1) (L.L.doorAcc_1) (L.S.Timegap) * - (S.L.doorSpeed_1) 
				{endif}
				(L.L.door_1) (L.L.doorSpeed_1) (L.S.Timegap) * + (S.L.door_1)
			{else}
				0 (S.L.doorSpeed_1)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_1) ! (L.L.doorSpeed_1) s0 abs 0.05 > (L.L.door_1) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_1) <
			{if}
				(L.L.doorSpeed_1) (L.L.doorAcc_1) (L.S.Timegap) * - (S.L.doorSpeed_1)
			{endif}
			(L.L.door_1) (L.L.doorSpeed_1) (L.S.Timegap) * + (S.L.door_1)
		{else}
			(L.L.doorSpeed_1) abs 0.05 > (L.L.door_1) 1 < || (L.L.doorTarget_1) &&
			{if}
				l0 (L.L.doorMaxSpeed_1) <
				{if}
					(L.L.doorSpeed_1) (L.L.doorAcc_1) (L.S.Timegap) * + (S.L.doorSpeed_1) 
				{endif}
				(L.L.door_1) (L.L.doorSpeed_1) (L.S.Timegap) * + (S.L.door_1)
			{else}
				0 (S.L.doorSpeed_1)
			{endif}
		{endif}
	{endif}
	(L.L.door_1) 1 >
	{if}
		(T.L.ev_doorhitopen_1)
		1 (S.L.door_1)
		(L.L.doorSpeed_1) /-/ (L.L.doorRefl_1) * (S.L.doorSpeed_1)
	{else}
		(L.L.door_1) 0 <
		{if}
			(T.L.ev_doorhitclose_1)
			0 (S.L.door_1)
			(L.L.doorSpeed_1) /-/ (L.L.doorRefl_1) * (S.L.doorSpeed_1)
		{endif}
	{endif}
{end}


{macro:DoorAftCalc}


	(L.L.bremse_halte_sw) !
	(L.L.door_3) 0 = &&
	(L.L.door_5) 0 = &&
	(L.L.door_7) 0 = &&
	(L.L.elec_busbar_main) ! ||
	(L.L.bremse_halte) &&
	{if}
		0 (S.L.bremse_halte) 
		0 (S.L.doorAftLastOpen) (S.L.doorAftLastOpen1) (S.L.doorAftLastOpen2)
		(T.L.ev_haltebremse_aus)
	{endif}

{end}

'--------------------------------------------------------------------------------


'--------------------------------------------------------------------------------

{macro:DoorAft_Open}

(L.L.bus_dooraft_sw)
		{if}
	
  	(L.L.PAX_Exit0_Req)
	(L.L.PAX_Exit1_Req) ||
	(L.L.bremse_halte) &&
   {if}
      (L.L.doorTarget_23) !
      (L.L.bremse_halte_sw) &&
      {if}
	(T.L.ev_doortriggeropen_2)
         1 (S.L.doorTarget_23)
         (C.L.door_druckluft)
         {if}
         (L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
         {endif}
      {endif}
      0 (S.L.doorAftLastOpen)      
   {endif}

	(L.L.PAX_Exit2_Req)
	(L.L.PAX_Exit3_Req) ||	
	(L.L.bremse_halte) &&
   {if}
      (L.L.doorTarget_45) !
      (L.L.bremse_halte_sw) &&
      		{if}
	(T.L.ev_doortriggeropen_5)
         1 (S.L.doorTarget_45)
	(T.L.ev_doortriggeropen_6)
         1 (S.L.doorTarget_67)
         (C.L.door_druckluft)
         {if}
         (L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
         {endif}
      {endif}
      0 (S.L.doorAftLastOpen1)
   {endif}
   
   	(L.L.PAX_Exit4_Req)
	(L.L.PAX_Exit5_Req) ||
	(L.L.bremse_halte) &&
   {if}		
      (L.L.doorTarget_67) !
      (L.L.bremse_halte_sw) &&
     		{if}
	(T.L.ev_doortriggeropen_6)
         1 (S.L.doorTarget_67)
         (C.L.door_druckluft)
         {if}
         (L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
         {endif}
      {endif}
      0 (S.L.doorAftLastOpen2)
   {endif}


(L.L.elec_busbar_main)
	{if}
		(L.L.bremse_halte)
		{if}
			(L.L.doorAftLastOpen) (L.S.Timegap) + (S.L.doorAftLastOpen)
			(L.L.doorAftLastOpen1) (L.S.Timegap) + (S.L.doorAftLastOpen1)
			(L.L.doorAftLastOpen2) (L.S.Timegap) + (S.L.doorAftLastOpen2)
		{endif}

		(L.L.doorTarget_23)
		(L.L.doorAftLastOpen) (C.L.doorAftOpenTime) > &&
		{if}
			(T.L.ev_doortriggerclose_2)
			0 (S.L.doorTarget_23)
			(C.L.door_druckluft)
			{if}
			(L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
			{endif}
		{endif}
	{endif}
		
		(L.L.doorTarget_45)
		(L.L.doorAftLastOpen1) (C.L.doorAftOpenTime) > &&
		{if}
			(T.L.ev_doortriggerclose_5)
			0 (S.L.doorTarget_45)
			(T.L.ev_doortriggerclose_6)
			0 (S.L.doorTarget_67)
			(C.L.door_druckluft)
			{if}
			(L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
			{endif}
		{endif}
	{endif}
	
		(L.L.doorTarget_67)
		(L.L.doorAftLastOpen2) (C.L.doorAftOpenTime) > &&
		{if}
			(T.L.ev_doortriggerclose_6)
			0 (S.L.doorTarget_67)
			(C.L.door_druckluft)
			{if}
			(L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
			{endif}			
		{endif}
	{endif}

{endif}
{end}

'--------------------------------------------------------------------------------

{macro:Door2_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_23)
		{if}
			(L.L.door_2) (F.L.door_2_opn_speed) (S.L.doorMaxSpeed_2)
			(L.L.door_2) (F.L.door_2_opn_speed_2) (S.L.door_2f)
		{else}
			(L.L.door_2) (F.L.door_2_cls_speed) (S.L.doorMaxSpeed_2)
			(L.L.door_2) (F.L.door_2_cls_speed_2) (S.L.door_2f)
		{endif}

		(C.L.bdoor_acc) (S.L.doorAcc_2)

		(L.L.doorTarget_23) ! (L.L.doorSpeed_2) s0 abs 0.05 > (L.L.door_2) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_2) <
			{if}
				(L.L.doorSpeed_2) (L.L.doorAcc_2) (L.S.Timegap) * - (S.L.doorSpeed_2)
			{else}
				(L.L.doorSpeed_2) (L.L.doorAcc_2) (L.S.Timegap) * + (S.L.doorSpeed_2)
			{endif}
			(L.L.door_2) (L.L.doorSpeed_2) (L.S.Timegap) * + (S.L.door_2)
		{else}
			(L.L.doorSpeed_2) abs 0.05 > (L.L.door_2) 1 < || (L.L.doorTarget_23) &&
			{if}
				l0 (L.L.doorMaxSpeed_2) <
				{if}
					(L.L.doorSpeed_2) (L.L.doorAcc_2) (L.S.Timegap) * + (S.L.doorSpeed_2) 
				{else}
					(L.L.doorSpeed_2) (L.L.doorAcc_2) (L.S.Timegap) * - (S.L.doorSpeed_2) 
				{endif}
				(L.L.door_2) (L.L.doorSpeed_2) (L.S.Timegap) * + (S.L.door_2)
			{else}
				0 (S.L.doorSpeed_2)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_23) ! (L.L.doorSpeed_2) s0 abs 0.05 > (L.L.door_2) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_2) <
			{if}
				(L.L.doorSpeed_2) (L.L.doorAcc_2) (L.S.Timegap) * - (S.L.doorSpeed_2)
			{endif}
			(L.L.door_2) (L.L.doorSpeed_2) (L.S.Timegap) * + (S.L.door_2)
		{else}
			(L.L.doorSpeed_2) abs 0.05 > (L.L.door_2) 1 < || (L.L.doorTarget_23) &&
			{if}
				l0 (L.L.doorMaxSpeed_2) <
				{if}
					(L.L.doorSpeed_2) (L.L.doorAcc_2) (L.S.Timegap) * + (S.L.doorSpeed_2) 
				{endif}
				(L.L.door_2) (L.L.doorSpeed_2) (L.S.Timegap) * + (S.L.door_2)
			{else}
				0 (S.L.doorSpeed_2)
			{endif}
		{endif}
	{endif}

	(L.L.door_2) 1 >
	{if}
		(T.L.ev_doorhitopen_2)
		1 (S.L.door_2)
		(L.L.doorSpeed_2) /-/ (L.L.doorRefl_2) * (S.L.doorSpeed_2)
	{else}
		(L.L.door_2) 0 <
		{if}
			(T.L.ev_doorhitclose_2)
			0 (S.L.door_2)
			(L.L.doorSpeed_2) /-/ (L.L.doorRefl_2) * (S.L.doorSpeed_2)
		{endif}
	{endif}
{end}

{macro:Door3_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_23)
		{if}
			(L.L.door_3) (F.L.door_3_opn_speed) (S.L.doorMaxSpeed_3)
			(L.L.door_3) (F.L.door_3_opn_speed_2) (S.L.door_3f)
		{else}
			(L.L.door_3) (F.L.door_3_cls_speed) (S.L.doorMaxSpeed_3)
			(L.L.door_3) (F.L.door_3_cls_speed_2) (S.L.door_3f)
		{endif}

		(C.L.bdoor_acc) (S.L.doorAcc_3)

		(L.L.doorTarget_23) ! (L.L.doorSpeed_3) s0 abs 0.05 > (L.L.door_3) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_3) <
			{if}
				(L.L.doorSpeed_3) (L.L.doorAcc_3) (L.S.Timegap) * - (S.L.doorSpeed_3)
			{else}
				(L.L.doorSpeed_3) (L.L.doorAcc_3) (L.S.Timegap) * + (S.L.doorSpeed_3)
			{endif}
			(L.L.door_3) (L.L.doorSpeed_3) (L.S.Timegap) * + (S.L.door_3)
		{else}
			(L.L.doorSpeed_3) abs 0.05 > (L.L.door_3) 1 < || (L.L.doorTarget_23) &&
			{if}
				l0 (L.L.doorMaxSpeed_3) <
				{if}
					(L.L.doorSpeed_3) (L.L.doorAcc_3) (L.S.Timegap) * + (S.L.doorSpeed_3) 
				{else}
					(L.L.doorSpeed_3) (L.L.doorAcc_3) (L.S.Timegap) * - (S.L.doorSpeed_3) 
				{endif}
				(L.L.door_3) (L.L.doorSpeed_3) (L.S.Timegap) * + (S.L.door_3)
			{else}
				0 (S.L.doorSpeed_3)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_23) ! (L.L.doorSpeed_3) s0 abs 0.05 > (L.L.door_3) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_3) <
			{if}
				(L.L.doorSpeed_3) (L.L.doorAcc_3) (L.S.Timegap) * - (S.L.doorSpeed_3)
			{endif}
			(L.L.door_3) (L.L.doorSpeed_3) (L.S.Timegap) * + (S.L.door_3)
		{else}
			(L.L.doorSpeed_3) abs 0.05 > (L.L.door_3) 1 < || (L.L.doorTarget_23) &&
			{if}
				l0 (L.L.doorMaxSpeed_3) <
				{if}
					(L.L.doorSpeed_3) (L.L.doorAcc_3) (L.S.Timegap) * + (S.L.doorSpeed_3) 
				{endif}
				(L.L.door_3) (L.L.doorSpeed_3) (L.S.Timegap) * + (S.L.door_3)
			{else}
				0 (S.L.doorSpeed_3)
			{endif}
		{endif}
	{endif}

	(L.L.door_3) 1 >
	{if}
		(T.L.ev_doorhitopen_3)
		1 (S.L.door_3)
		(L.L.doorSpeed_3) /-/ (L.L.doorRefl_3) * (S.L.doorSpeed_3)
	{else}
		(L.L.door_3) 0 <
		{if}
			(T.L.ev_doorhitclose_3)
			0 (S.L.door_3)
			(L.L.doorSpeed_3) /-/ (L.L.doorRefl_3) * (S.L.doorSpeed_3)
		{endif}
	{endif}

{end}

{macro:Door4_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_45)
		{if}
			(L.L.door_4) (F.L.door_4_opn_speed) (S.L.doorMaxSpeed_4)
			(L.L.door_4) (F.L.door_4_opn_speed_2) (S.L.door_4f)
		{else}
			(L.L.door_4) (F.L.door_4_cls_speed) (S.L.doorMaxSpeed_4)
			(L.L.door_4) (F.L.door_4_cls_speed_2) (S.L.door_4f)
		{endif}

		(C.L.bdoor_acc) (S.L.doorAcc_4)

		(L.L.doorTarget_45) ! (L.L.doorSpeed_4) s0 abs 0.05 > (L.L.door_4) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_3) <
			{if}
				(L.L.doorSpeed_4) (L.L.doorAcc_4) (L.S.Timegap) * - (S.L.doorSpeed_4)
			{else}
				(L.L.doorSpeed_4) (L.L.doorAcc_4) (L.S.Timegap) * + (S.L.doorSpeed_4)
			{endif}
			(L.L.door_4) (L.L.doorSpeed_4) (L.S.Timegap) * + (S.L.door_4)
		{else}
			(L.L.doorSpeed_4) abs 0.05 > (L.L.door_4) 1 < || (L.L.doorTarget_45) &&
			{if}
				l0 (L.L.doorMaxSpeed_4) <
				{if}
					(L.L.doorSpeed_4) (L.L.doorAcc_4) (L.S.Timegap) * + (S.L.doorSpeed_4) 
				{else}
					(L.L.doorSpeed_4) (L.L.doorAcc_4) (L.S.Timegap) * - (S.L.doorSpeed_4) 
				{endif}
				(L.L.door_4) (L.L.doorSpeed_4) (L.S.Timegap) * + (S.L.door_4)
			{else}
				0 (S.L.doorSpeed_4)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_45) ! (L.L.doorSpeed_4) s0 abs 0.05 > (L.L.door_4) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_4) <
			{if}
				(L.L.doorSpeed_4) (L.L.doorAcc_4) (L.S.Timegap) * - (S.L.doorSpeed_4)
			{endif}
			(L.L.door_4) (L.L.doorSpeed_4) (L.S.Timegap) * + (S.L.door_4)
		{else}
			(L.L.doorSpeed_4) abs 0.05 > (L.L.door_4) 1 < || (L.L.doorTarget_45) &&
			{if}
				l0 (L.L.doorMaxSpeed_4) <
				{if}
					(L.L.doorSpeed_4) (L.L.doorAcc_4) (L.S.Timegap) * + (S.L.doorSpeed_4) 
				{endif}
				(L.L.door_4) (L.L.doorSpeed_4) (L.S.Timegap) * + (S.L.door_4)
			{else}
				0 (S.L.doorSpeed_4)
			{endif}
		{endif}
	{endif}

	(L.L.door_4) 1 >
	{if}
		(T.L.ev_doorhitopen_4)
		1 (S.L.door_4)
		(L.L.doorSpeed_4) /-/ (L.L.doorRefl_4) * (S.L.doorSpeed_4)
	{else}
		(L.L.door_4) 0 <
		{if}
			(T.L.ev_doorhitclose_4)
			0 (S.L.door_4)
			(L.L.doorSpeed_4) /-/ (L.L.doorRefl_4) * (S.L.doorSpeed_4)
		{endif}
	{endif}

{end}

{macro:Door5_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_45)
		{if}
			(L.L.door_5) (F.L.door_5_opn_speed) (S.L.doorMaxSpeed_5)
			(L.L.door_5) (F.L.door_5_opn_speed_2) (S.L.door_5f)
		{else}
			(L.L.door_5) (F.L.door_5_cls_speed) (S.L.doorMaxSpeed_5)
			(L.L.door_5) (F.L.door_5_cls_speed_2) (S.L.door_5f)
		{endif}

		(C.L.bdoor_acc) (S.L.doorAcc_5)

		(L.L.doorTarget_45) ! (L.L.doorSpeed_5) s0 abs 0.05 > (L.L.door_5) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_5) <
			{if}
				(L.L.doorSpeed_5) (L.L.doorAcc_5) (L.S.Timegap) * - (S.L.doorSpeed_5)
			{else}
				(L.L.doorSpeed_5) (L.L.doorAcc_5) (L.S.Timegap) * + (S.L.doorSpeed_5)
			{endif}
			(L.L.door_5) (L.L.doorSpeed_5) (L.S.Timegap) * + (S.L.door_5)
		{else}
			(L.L.doorSpeed_5) abs 0.05 > (L.L.door_5) 1 < || (L.L.doorTarget_45) &&
			{if}
				l0 (L.L.doorMaxSpeed_5) <
				{if}
					(L.L.doorSpeed_5) (L.L.doorAcc_5) (L.S.Timegap) * + (S.L.doorSpeed_5) 
				{else}
					(L.L.doorSpeed_5) (L.L.doorAcc_5) (L.S.Timegap) * - (S.L.doorSpeed_5) 
				{endif}
				(L.L.door_5) (L.L.doorSpeed_5) (L.S.Timegap) * + (S.L.door_5)
			{else}
				0 (S.L.doorSpeed_5)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_45) ! (L.L.doorSpeed_5) s0 abs 0.05 > (L.L.door_5) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_5) <
			{if}
				(L.L.doorSpeed_5) (L.L.doorAcc_5) (L.S.Timegap) * - (S.L.doorSpeed_5)
			{endif}
			(L.L.door_5) (L.L.doorSpeed_5) (L.S.Timegap) * + (S.L.door_5)
		{else}
			(L.L.doorSpeed_5) abs 0.05 > (L.L.door_5) 1 < || (L.L.doorTarget_45) &&
			{if}
				l0 (L.L.doorMaxSpeed_5) <
				{if}
					(L.L.doorSpeed_5) (L.L.doorAcc_5) (L.S.Timegap) * + (S.L.doorSpeed_5) 
				{endif}
				(L.L.door_5) (L.L.doorSpeed_5) (L.S.Timegap) * + (S.L.door_5)
			{else}
				0 (S.L.doorSpeed_5)
			{endif}
		{endif}
	{endif}

	(L.L.door_5) 1 >
	{if}
		(T.L.ev_doorhitopen_5)
		1 (S.L.door_5)
		(L.L.doorSpeed_5) /-/ (L.L.doorRefl_5) * (S.L.doorSpeed_5)
	{else}
		(L.L.door_5) 0 <
		{if}
			(T.L.ev_doorhitclose_5)
			0 (S.L.door_5)
			(L.L.doorSpeed_5) /-/ (L.L.doorRefl_5) * (S.L.doorSpeed_5)
		{endif}
	{endif}

{end}

{macro:Door7_Calc}
	(C.L.electric_doors)
	{if}
		(L.L.doorTarget_67)
		{if}
			(L.L.door_7) (F.L.door_7_opn_speed) (S.L.doorMaxSpeed_7)
			(L.L.door_7) (F.L.door_7_opn_speed_2) (S.L.door_7f)
		{else}
			(L.L.door_7) (F.L.door_7_cls_speed) (S.L.doorMaxSpeed_7)
			(L.L.door_7) (F.L.door_7_cls_speed_2) (S.L.door_7f)
		{endif}

		(C.L.bdoor_acc) (S.L.doorAcc_7)

		(L.L.doorTarget_67) ! (L.L.doorSpeed_7) s0 abs 0.05 > (L.L.door_7) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_7) <
			{if}
				(L.L.doorSpeed_7) (L.L.doorAcc_7) (L.S.Timegap) * - (S.L.doorSpeed_7)
			{else}
				(L.L.doorSpeed_7) (L.L.doorAcc_7) (L.S.Timegap) * + (S.L.doorSpeed_7)
			{endif}
			(L.L.door_7) (L.L.doorSpeed_7) (L.S.Timegap) * + (S.L.door_7)
		{else}
			(L.L.doorSpeed_7) abs 0.05 > (L.L.door_7) 1 < || (L.L.doorTarget_67) &&
			{if}
				l0 (L.L.doorMaxSpeed_7) <
				{if}
					(L.L.doorSpeed_7) (L.L.doorAcc_7) (L.S.Timegap) * + (S.L.doorSpeed_7) 
				{else}
					(L.L.doorSpeed_7) (L.L.doorAcc_7) (L.S.Timegap) * - (S.L.doorSpeed_7) 
				{endif}
				(L.L.door_7) (L.L.doorSpeed_7) (L.S.Timegap) * + (S.L.door_7)
			{else}
				0 (S.L.doorSpeed_7)
			{endif}
		{endif}
	{else}
		(L.L.doorTarget_67) ! (L.L.doorSpeed_7) s0 abs 0.05 > (L.L.door_7) 0 > || && 
		{if}
			l0 /-/ (L.L.doorMaxSpeed_7) <
			{if}
				(L.L.doorSpeed_7) (L.L.doorAcc_7) (L.S.Timegap) * - (S.L.doorSpeed_7)
			{endif}
			(L.L.door_7) (L.L.doorSpeed_7) (L.S.Timegap) * + (S.L.door_7)
		{else}
			(L.L.doorSpeed_7) abs 0.05 > (L.L.door_7) 1 < || (L.L.doorTarget_67) &&
			{if}
				l0 (L.L.doorMaxSpeed_7) <
				{if}
					(L.L.doorSpeed_7) (L.L.doorAcc_7) (L.S.Timegap) * + (S.L.doorSpeed_7) 
				{endif}
				(L.L.door_7) (L.L.doorSpeed_7) (L.S.Timegap) * + (S.L.door_7)
			{else}
				0 (S.L.doorSpeed_7)
			{endif}
		{endif}
	{endif}

	(L.L.door_7) 1 >
	{if}
		(T.L.ev_doorhitopen_7)
		1 (S.L.door_7)
		(L.L.doorSpeed_7) /-/ (L.L.doorRefl_7) * (S.L.doorSpeed_7)
	{else}
		(L.L.door_7) 0 <
		{if}
			(T.L.ev_doorhitclose_7)
			0 (S.L.door_7)
			(L.L.doorSpeed_7) /-/ (L.L.doorRefl_7) * (S.L.doorSpeed_7)
		{endif}
	{endif}

{end}


{macro:trg_bus_doorfront0}

	(L.L.doorTarget_0) ! (S.L.doorTarget_0) 
	{if}
		(T.L.ev_doortriggeropen_0)
	{else}
		(T.L.ev_doortriggerclose_0)
	{endif}
		(C.L.door_druckluft)
		{if}
		(L.L.bremse_p_Tank04) 100000 - 0.98 * 100000 + (S.L.bremse_p_Tank04)
		{endif}
{end}

{macro:trg_bus_doorfront1}

	(L.L.doorTarget_1) ! (S.L.doorTarget_1) 
	{if}
		(T.L.ev_doortriggeropen_1)
	{else}
		(T.L.ev_doortriggerclose_1)
	{endif}	
		(C.L.door_druckluft)
		{if}
		(L.L.bremse_p_Tank04) 100000 - 0.98 * 100000 + (S.L.bremse_p_Tank04)
		{endif}
{end}

{macro:trg_bus_doorback23}

	(L.L.doorTarget_23) ! (S.L.doorTarget_23) 
	{if}
		(T.L.ev_doortriggeropen_2)
	{else}
		(T.L.ev_doortriggerclose_2)
	{endif}	
		(C.L.door_druckluft)
		{if}
		(L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
		{endif}
{end}

{macro:trg_bus_doorfront5}

	(L.L.doorTarget_45) ! (S.L.doorTarget_45) 
	{if}
		(T.L.ev_doortriggeropen_5)
	{else}
		(T.L.ev_doortriggerclose_5)
	{endif}	
		(C.L.door_druckluft)
		{if}
		(L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
		{endif}
{end}

{macro:trg_bus_doorfront6}

	(L.L.doorTarget_67) ! (S.L.doorTarget_67)
	{if}
		(T.L.ev_doortriggeropen_6)
	{else}
		(T.L.ev_doortriggerclose_6)
	{endif}	

		(C.L.door_druckluft)
		{if}
		(L.L.bremse_p_Tank04) 100000 - 0.96 * 100000 + (S.L.bremse_p_Tank04)
		{endif}
	
{end}

{macro:trg_bus_dooraft}
	(L.L.bremse_halte_sw) ! (S.L.bremse_halte_sw)
		

	(L.L.bremse_halte_sw)
	{if}
		(T.L.ev_haltebremse_sw_an)
	{else}
		(T.L.ev_haltebremse_sw_aus)
	{endif}
{end}

{macro:trg_bus_20h-switch}
	(L.L.door_20h_sw) ! (S.L.door_20h_sw)
	
	(L.L.door_20h_sw)
	{if}
		(T.L.ev_haltebremse_sw_an)
	{else}
		(T.L.ev_haltebremse_sw_aus)
	{endif}	
{end}

{trigger:bus_dooraft_switch}
	(L.L.bus_dooraft_sw) ! (S.L.bus_dooraft_sw)
	
	(L.L.bus_dooraft_sw)
	{if}
		(T.L.ev_haltebremse_sw_an)
	{else}
		(T.L.ev_haltebremse_sw_aus)
	{endif}	
{end}