
[newcurve]
ERA_lock

[pnt]
0
0

[pnt]
3
1

[const]
ERA_distort_coeff
0.012

[const]
auto_HST_bremse
0

[const]
kneel_time_up
3.5

[const]
kneel_time_down
3.5

[const]
kneel_target_pressure
500

Max braking force
[const]
max_bremskraft
120000

[const]
bremse_ABS
1

Mass flow of the compressor in kg per engine revolution
[const]
bremse_m_kompressor
0.00065

Volume [m³] Air line compressor protection valve
[const]
bremse_V_leitung01
0.002

Volume [m³] Air line circuit 1 + 2 to 3 + 4
[const]
bremse_V_leitung02
0.002

Cross-section area Check valves for filling line circles 3 + 4
[const]
bremse_A_Rueckschlagventil_1
0.00003

Volume [m³] air tank circle 1 (HA)
[const]
bremse_V_tank01
0.04

Volume [m³] air tank circle 2 (VA)
[const]
bremse_V_tank02
0.04

Volume [m³] air tank circle 3 (FBA)
[const]
bremse_V_tank03
0.04

Volume [m³] air tank circle 4 (Suspension+doors+HBA)
[const]
bremse_V_tank04
0.04

Volume brake cylinder HA
[const]
bremse_V_Brzyl_HA
0.0025

Volume brake cylinder HA right
[const]
bremse_V_Brzyl_HA_R
0.00125

Volume brake cylinder HA left
[const]
bremse_V_Brzyl_HA_L
0.00125

Volume brake cylinder LA
[const]
bremse_V_Brzyl_LA
0.0025

Volume brake cylinder LA rechts
[const]
bremse_V_Brzyl_LA_R
0.00125

Volume brake cylinder LA
[const]
bremse_V_Brzyl_LA_L
0.00125

Volume brake cylinder MA
[const]
bremse_V_Brzyl_MA
0.0025

Volume brake cylinder MA right
[const]
bremse_V_Brzyl_MA_R
0.00125

Volume brake cylinder MA left
[const]
bremse_V_Brzyl_MA_L
0.00125

Volume brake cylinder VA
[const]
bremse_V_Brzyl_VA
0.0025

Volume brake cylinder VA right
[const]
bremse_V_Brzyl_VA_R
0.00125

Volume brake cylinder VA left
[const]
bremse_V_Brzyl_VA_L
0.00125

Volume brake cylinder FBA
[const]
bremse_V_brzyl_FBA
0.02

Volume air bag 0 R
[const]
bremse_V_balg_0_R
0.005

Volume air bag 0 L
[const]
bremse_V_balg_0_L
0.005

Volume air bag 1 R
[const]
bremse_V_balg_1_R
0.01

Volume air bag 1 L
[const]
bremse_V_balg_1_L
0.01

Volume air bag 2 R
[const]
bremse_V_balg_2_R
0.01

Volume air bag 2 L
[const]
bremse_V_balg_2_L
0.01

Volume air bag 3 R
[const]
bremse_V_balg_3_R
0.01

Volume air bag 3 L
[const]
bremse_V_balg_3_L
0.01

Gas constant * Average temperature
[const]
RT_Luft
84091

Operating pressure stop brake
[const]
bremse_pmax_halte
450000

Opening pressure overflow valve circuit 1
[const]
bremse_UeVentil_1_oeffnungsdruck
750000

Closing pressure overflow valve circuit 1
[const]
bremse_UeVentil_1_schliessdruck
600000

Opening pressure overflow valve circuit 2
[const]
bremse_UeVentil_2_oeffnungsdruck
750000

Closing pressure overflow valve circuit 2
[const]
bremse_UeVentil_2_schliessdruck
600000

Opening pressure overflow valve circuit 3
[const]
bremse_UeVentil_3_oeffnungsdruck
750000

Closing pressure overflow valve circuit 3
[const]
bremse_UeVentil_3_schliessdruck
600000

Opening pressure overflow valve circuit 4
[const]
bremse_UeVentil_4_oeffnungsdruck
750000

Closing pressure overflow valve circuit 4
[const]
bremse_UeVentil_4_schliessdruck
600000

[newcurve]
Bremskraft_FBA

[pnt]
100000
35000

[pnt]
650000
0

[pnt]
10000000
0

Setpoint for level control
[const]
bremse_level_setpoint
-0.105


Setpoint for axle suspension
[const]
Axle_Spring_0_high
0.5
    0.45

[const]
Axle_Spring_0_low
0.35

[const]
Axle_Spring_1_high
0.5
    0.46

[const]
Axle_Spring_1_low
0.35

[const]
Axle_Spring_2_high
0.5
    0.45

[const]
Axle_Spring_2_low
0.35

[const]
Axle_Spring_3_high
0.5
    0.45

[const]
Axle_Spring_3_low
0.35

[const]
Axle_Spring_anheben_high
1

[const]
Axle_Spring_anheben_low
0.3

Control tolerance for electronic level control:
[const]
bremse_levelcontrol_tolerance
0.015

Simulation of the pulse behavior of the control valves when approaching the setpoint (avoidance of instabilities)
[newcurve]
bremse_suspension_regulatorcurve

[pnt]
-0.03
1

[pnt]
-0.01
0.15

[pnt]
0
0.2

[pnt]
0.005
0.5

[pnt]
0.01
1

Test leak size
[const]
bremse_A_Leck
0.0001
