[const]
engine_J
3

[const]
engine_speedcontrol
1

[newcurve]
max_speed

[pnt]
57
1

[pnt]
60
0

------------------------
Desligamento automatico do motor 
------------------------

[const]
engine_auto_turnoff
1

[const]
engine_turnoff_warn_limit
170

[const]
engine_turnoff_timer_limit
200

-----------------------

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
560

[const]
engine_governed_max_RPM
2170

[const]
engine_governed_max_RPM_eco
1500

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350


[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4


[const]
engine_starterM
1000

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[const]
torque_apex_at_RPM
1300

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
600
1000

[pnt]
700
1350

[pnt]
800
1450

[pnt]
900
1550

[pnt]
1000
1590

[pnt]
1100
1610

[pnt]
1200
1600

[pnt]
1300
1585

[pnt]
1400
1575

[pnt]
1500
1550

[pnt]
1600
1500

[pnt]
1700
1440

[pnt]
1800
1375

[pnt]
1900
1300

[pnt]
2000
1300

[pnt]
2100
900

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
475
300

[pnt]
575
0

[pnt]
675
-100

[pnt]
1000
-200

[pnt]
2200
-300

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
300
0

[pnt]
565
0

[pnt]
600
-220

[pnt]
900
-800

[pnt]
1400
-800

[pnt]
1700
-600

[pnt]
2000
-420

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.52

[pnt]
1100
0.73

[pnt]
1190
0.78

[pnt]
1450
0.7

[pnt]
1700
0.53

[pnt]
2300
0.3

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1

[const]
engine_fuel_value
11.5
    9.97
    Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
500

[const]
engine_adblue_capacity
35



[const]
luefterthermostat_opn
88

[const]
luefterthermostat_cls
86

[const]
kuehlerthermostat_opn
84

[const]
kuehlerthermostat_cls
81

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100

[pnt]
125
0

[newcurve]
smoke_fire

[pnt]
0
0

[pnt]
120
0

[pnt]
125
100

[const]
engine_overheat_toleranz
50


[const]
engine_Qrate_engine_factor
0.85

[const]
engine_Qrate_cooling_factor
950

[const]
engine_Qrate_fan_factor
1.155

[const]
engine_Qrate_veloc_factor_basic
250

[const]
engine_Qrate_veloc_factor
2

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000


[newcurve]
engine_turbo_RPM_factor

[pnt]
0
0

[pnt]
500
0.6

[pnt]
1200
1.4

[pnt]
1600
1.4

[pnt]
2000
1.7


[newcurve]
engine_turbo_throttle_factor

[pnt]
0
0.5

[pnt]
1
1

[newcurve]
engine_turbo_boost

[pnt]
0
1

[pnt]
70
1

[pnt]
90
1

[pnt]
100
1