[const]
engine_J
3

[const]
engine_speedcontrol
1

[newcurve]
max_speed

[pnt]
60
1

[pnt]
61
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
590

[const]
engine_governed_limited_RPM
1500

[const]
engine_governed_max_RPM
2500

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350


[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05

[const]
engine_RPM_ign_cold
150

[const]
engine_RPM_ign_warm
100

	Zeit [s], wie lange er "orgelt", wenn er gerade so die untere, "warme" Grenzdrehzahl erreicht:

[const]
engine_RPM_ign_time2warm
4


[const]
engine_starterM
1000

[const]
engine_starter_n_halbwert
67

[const]
engine_startering_sound_n_max
450

Mindeststrom, der immer durch den Starter fließt

[const]
engine_starter_minI
300

Ampere/Nm:

[const]
engine_starter_Ifaktor
0.5

[const]
torque_apex_at_RPM
1200

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
600
700

[pnt]
700
750

[pnt]
800
800

[pnt]
900
850

[pnt]
1000
900

[pnt]
1100
900

[pnt]
1600
900

[pnt]
1700
880

[pnt]
1800
860

[pnt]
1900
840

[pnt]
2000
820

[pnt]
2100
810

[pnt]
2200
800

[pnt]
2500
600

[pnt]
2800
495

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
475
300

[pnt]
575
0

[pnt]
675
-100

[pnt]
1000
-200

[pnt]
2200
-300

[newcurve]
engine_M_brake

[pnt]
50
0

[pnt]
300
0

[pnt]
565
0

[pnt]
600
-120

[pnt]
900
-300

[pnt]
1400
-400

[pnt]
1700
-500

[pnt]
2000
-320

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
1100
0.80

[pnt]
1450
0.80

[pnt]
1700
0.46

[pnt]
2300
0.3

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1

[const]
engine_fuel_value
11.5
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
300

[const]
engine_adblue_capacity
35

[const]
luefterthermostat_opn
88

[const]
luefterthermostat_cls
86

[const]
kuehlerthermostat_opn
84

[const]
kuehlerthermostat_cls
81

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100

[pnt]
125
0

[newcurve]
smoke_fire

[pnt]
0
0

[pnt]
120
0

[pnt]
125
100

[const]
engine_overheat_toleranz
50


[const]
engine_Qrate_engine_factor
1.05

[const]
engine_Qrate_cooling_factor
900

[const]
engine_Qrate_fan_factor
1.1

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
3

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000


[newcurve]
engine_turbo_RPM_factor

[pnt]
0
0

[pnt]
500
0.5

[pnt]
1200
0.7

[pnt]
1600
0.9

[pnt]
2000
1


[newcurve]
engine_turbo_throttle_factor

[pnt]
0
0.5

[pnt]
1
1

[newcurve]
engine_turbo_boost

[pnt]
0
1

[pnt]
70
1.03

[pnt]
90
1.05

[pnt]
100
1.08