[const]
engine_J
3.5


[const]
engine_J_max
2.2

[const]
engine_J_in
4

[const]
engine_consumption_curve_available
1

[const]
smoke_control
0


[const]
engine_ECM_Throttle
0




[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
0

[const]
speedgov
105

[const]
turbochaged
1

[const]
rpmgov
2200

[const]
engine_governed_idle_RPM
650

[const]
engine_power_idle
25124

[const]
engine_coldM
-300



[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
0
120


[pnt]
800
195


[pnt]
1100
190


[pnt]
1900
211


[pnt]
2800
255

[pnt]
4800
415

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
540

[pnt]
600
600

[pnt]
800
1030

[pnt]
1000
1050

[pnt]
1300
1050

[pnt]
1700
1000

[pnt]
1900
960

[pnt]
2300
750

[pnt]
2500
0




[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
350
350

[pnt]
550
250

[pnt]
650
0

[pnt]
700
-50

[pnt]
800
-106


[pnt]
1000
-176

[pnt]
1500
-206


[pnt]
3000
-304

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
1




[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2


[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_fuel_value
11.8
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000







[newcurve]
governor


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
0

[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0


[newcurve]
torque_map

[pnt]
-100
1

[pnt]
100
0


Pressure Ratio starts at 1:1, so an second  value at 0 would yield a pressure ratio of 1:1 or 14.7 PSI Non Aspirate Pressure with 0 PSI turbocharge boost.
[newcurve]
turbo_exhaust_flow

[pnt]
0
0

[pnt]
100
1

[pnt]
200
6.2


[pnt]
400
19.11

[pnt]
600
32.4

[pnt]
800
44.1


[newcurve]
throttle_map

[pnt]
0
0

[pnt]
1100
2

[pnt]
1300
2




[const]
engine_volumetric_efficiency
77

Value in mm
[const]
turbo_compressor_wheel_size
70


[const]
turbo_min_psi
0


[const]
turbo_max_psi
21.75


number of liters the engine has (CID) this helps calculate the spool rate of the turbocharger

[const]
engine_CID
11.97


[newcurve]
turbo_spool

[pnt]
0
0

[pnt]
30
8



[newcurve]
turbo_spool_oj

[pnt]
0
0.5

[pnt]
14.7
1



[newcurve]
engine_govern_balance


[pnt]
600
1

[pnt]
700
0


[newcurve]
asa

[pnt]
0.6
1.3

[pnt]
0.96
1

[newcurve]
Torque_Requested_Map

[pnt]
0.5
2


[pnt]
0.98
1

[newcurve]
engine_brake_fadin

[pnt]
0
1


[pnt]
0.25
1
