[const]
engine_J
2.25

[const]
engine_e-gas
1

[const]
speedgov
69

[const]
rpmgov
2750

[const]
engine_governed_idle_RPM
700

[const]
engine_Year
2013

[const]
engine_NoElecMadeinchina
0

[const]
engine_ElecCtrl
1

[const]
eng_L
4.255



[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
315

[pnt]
400
325

[pnt]
500
350

[pnt]
600
375

[pnt]
700
400

[pnt]
800
425

[pnt]
900
450

[pnt]
1000
500

[pnt]
1200
560

[pnt]
1400
590

[pnt]
1500
600

[pnt]
1600
600

[pnt]
1800
560

[pnt]
2000
550

[pnt]
2200
510

[pnt]
2400
470

[pnt]
2500
450

[pnt]
2750
225

[pnt]
2875
112.5

[pnt]
3000
0


[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
315

[pnt]
595
373.8

[pnt]
630
229.5

[pnt]
665
50

[pnt]
700
0

[pnt]
736
-4.5

[pnt]
880
-34

[pnt]
1060
-80

[pnt]
1780
-148

[pnt]
2140
-182

[pnt]
2500
-227

[pnt]
2750
-272

[pnt]
2875
-327

[pnt]
3000
-392

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
300
1

[pnt]
700
1

[pnt]
1600
0.99

[pnt]
2500
0.98

[pnt]
2750
0.75

[pnt]
2875
0.5

[newcurve]
engine_efficiency_throttle

[pnt]
0
0

[pnt]
0.2
0.2

[pnt]
0.85
0.85

[pnt]
1
1.05

[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_consumption_curve_available
1

[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
50
300

[pnt]
200
262.5

[pnt]
400
243.8

[pnt]
600
234.4

[pnt]
800
229.7

[pnt]
1000
225

[pnt]
1200
213

[pnt]
1400
207

[pnt]
1600
204

[pnt]
1800
203

[pnt]
2000
203

[pnt]
2200
205

[pnt]
2400
210

[pnt]
2500
218

[pnt]
2750
239.8

[pnt]
2875
261.6

[pnt]
3000
283.4

[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87.5

[const]
kuehlerthermostat_opn
87

[const]
kuehlerthermostat_cls
85

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
108
0

[pnt]
120
100

[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
400

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000

First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.98

[pnt]
30
1.01

[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0

[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency

[pnt]
550
1

[pnt]
1000
1.1

[newcurve]
turbo_engine_rpm_max_psi

[pnt]
500
0

[pnt]
750
20

[pnt]
1200
30

[newcurve]
turbo_inertia

[pnt]
0
3

[pnt]
10
30

[pnt]
30
90

[newcurve]
turbo_inertia_dec

[pnt]
0
0.5

[pnt]
30
30

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0

[pnt]
1
1

[newcurve]
governor

[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
-0.01

[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0

[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
10
2

[newcurve]
engine_efficiency_random

[pnt]
1
0.5

[pnt]
3
0.75

[pnt]
6
1

[newcurve]
engine_efficiency_random2

[pnt]
1
0.1

[pnt]
6
0.5

[pnt]
13
0.5

[pnt]
20
1
