[const]
engine_J
3.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
engine_governed_idle_RPM
600

[const]
engine_power_idle
15124

[const]
engine_coldM
-300

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
592
450

[pnt]
1300
1220

[pnt]
1600
1146

[pnt]
2000
1030

[pnt]
2200
915

[pnt]
2300
0


Speed Govern - In KPH 

[const]
speedgov
97


[const]
rpmgov
2260

[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-150

[pnt]
1000
-150

[pnt]
2500
-150

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1



[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000

[newcurve]
governor
[pnt]
-1000
1


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
-0.01

First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.35

[pnt]
30
0.35


[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0

[pnt]
1
30




[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
2

[pnt]
1300
30


[newcurve]
turbo_interia

[pnt]
0
1

[pnt]
10
10

[pnt]
30
30


[newcurve]
turbo_interia_dec

[pnt]
0
0

[pnt]
5
2

[pnt]
10
5

[pnt]
30
30