[const]
engine_J
3.5

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

Speed Govern - In KPH 

[const]
speedgov
150


[const]
rpmgov
2000


[const]
engine_governed_idle_RPM
550

[const]
engine_power_idle
15124

[const]
engine_coldM
-300

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
370

[pnt]
592
1000


[pnt]
800
1400

[pnt]
1000
1550

[pnt]
1100
1600

[pnt]
1400
1550

[pnt]
1750
1400

[pnt]
2000
1250

[pnt]
2100
0


[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-150

[pnt]
1000
-300

[pnt]
2500
-300

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.4

[pnt]
1000
0.2

[pnt]
1400
0.185

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2

[const]
engine_fuel_value
10.8

Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000



First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.69


[pnt]
30
1



[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0

[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency


[pnt]
850
0.50

[pnt]
1000
1.00


[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
2

[pnt]
850
10

[pnt]
1000
30


[newcurve]
governor

[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
-0.01

[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0


First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.60


[pnt]
30
1



[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0

[pnt]
0.85
25

[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency

[pnt]
750
0.50

[pnt]
1000
1.00


[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
2

[pnt]
850
10

[pnt]
1000
30


[newcurve]
turbo_inertia

[pnt]
0
1

[pnt]
10
30


[newcurve]
turbo_inertia_dec

[pnt]
0
0

[pnt]
5
2

[pnt]
10
5

[pnt]
30
30

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0


[pnt]
1
1


[newcurve]
engine_braking

[pnt]
0
1

[pnt]
0.2
0

[newcurve]
engine_airflow

[pnt]
0
0.15

[pnt]
5
0.5


[pnt]
100
2