Getriebeversion: 
1: Retarder nicht im 1. Gang, keine Neutralschaltung
2: Retarder im 1. Gang, Neutralschaltung
3: Retarder nicht im 1. Gang, Neutralschaltung
[const]
antrieb_getr_version
3

Zeit für den Wechsel zwischen Retarder und Traktion (nur bei Getriebeversion 2)
[const]
antrieb_retarder_changetime
0.6

Mindestzeit, die eingekuppelt sein muss, bevor Neutralschaltung greift
[const]
antrieb_gear_engaged_mintime
2

Geschwindigkeit, unterhalb der die Neutralschaltung greift
[const]
antrieb_neutral_maxspeed
70

Bremsdruck in Pa, ab dem Neutralschaltung greift
[const]
antrieb_neutral_brakepressure
170000

[const]
CVT_Mode_A_lo
3.7

[const]
CVT_Mode_A_hi
1.7



[const]
CVT_Mode_B_lo
3.7

[const]
CVT_Mode_B_hi
0.5

[const]
antrieb_kuppl_M_up_max
1100

[const]
antrieb_kuppl_M_up_min
400

[const]
antrieb_kuppl_M_dn_max
1100

[const]
antrieb_kuppl_M_dn_min
500

[const]
antrieb_getr_ratio1
1.36

[const]
antrieb_getr_ratio2
1.36

[const]
antrieb_getr_ratio3
1.0

[const]
antrieb_i_achse
5.74


Die folgenden Werte beziehen sich auf die Drehzahl der Kardanwelle und sind somit unabhängig von Achsübersetzung und Reifengröße!
km/h zu Wellendrehzahl (Raddurchmesser=1.03, i_achse=5.74 =>Faktor 29.56

[const]
antrieb_getr_autoSwUpMinSpd1
820

[const]
antrieb_getr_autoSwUpMaxSpd1
820

[const]
antrieb_getr_autoSwUpkickdnSpd1
820

[const]
antrieb_getr_autoSwDnMinSpd2
300

[const]
antrieb_getr_autoSwDnMaxSpd2
300

[const]
antrieb_getr_autoSwDnkickdnSpd2
650

[const]
antrieb_getr_autoSwUpMinSpd2
1040
1300

[const]
antrieb_getr_autoSwUpMaxSpd2
1180
1300

[const]
antrieb_getr_autoSwUpkickdnSpd2
1537

[const]
antrieb_getr_autoSwDnMinSpd3
800

[const]
antrieb_getr_autoSwDnMaxSpd3
1040

[const]
antrieb_getr_autoSwDnkickdnSpd3
1408

[const]
antrieb_wandler_fillrate
1000


[const]
retarder_min_einschaltspeed
502

[const]
antrieb_retarder_startdelay
0.2

[newcurve]
retarder_stufe1
[pnt]
0
0
[pnt]
10
194
[pnt]
20
388
[pnt]
30
407
[pnt]
40
485
[pnt]
50
641
[pnt]
60
854
[pnt]
70
990
[pnt]
80
1165

[newcurve]
retarder_stufe2
[pnt]
0
0
[pnt]
10
291
[pnt]
20
582
[pnt]
30
874
[pnt]
40
1019
[pnt]
50
1165
[pnt]
60
1262
[pnt]
70
1359
[pnt]
80
1456

[newcurve]
retarder_stufe3
[pnt]
0
0
[pnt]
10
291
[pnt]
20
582
[pnt]
30
1068
[pnt]
40
1554
[pnt]
50
1845
[pnt]
60
1942
[pnt]
70
1991
[pnt]
80
2039


[newcurve]
accel_1
[pnt]
0.25
1


[pnt]
1
0


[newcurve]
traction_throttle

[pnt]
0
0.1


[pnt]
0.85
1


[newcurve]
xxx

[pnt]
-0.2
0.01


[pnt]
0.85
1

[newcurve]
hybrid_vel


[pnt]
0
1


[pnt]
32
0.2


[const]
antrieb_gangwahlzeit
0.5

[const]
antrieb_neutralwahlzeit
0.1

[newcurve]
antrieb_wandler_lambda

[pnt]
-2
50

[pnt]
0
8.5

[pnt]
0.5
3.1

[pnt]
0.7
0

[newcurve]
antrieb_wandler_my

[pnt]
0
5
4.65

[pnt]
0.6
1.4

[pnt]
0.7
0


[newcurve]
antrieb_reverse_torque_reduction

[pnt]
-220
0

[pnt]
0
1



[newcurve]
antrieb_wandler_lambda_r

[pnt]
0.2
-12

[pnt]
0.5
-8

[pnt]
1
-4

[pnt]
1.42857
0


[newcurve]
antrieb_wandler_my_r

[pnt]
0.2
5

[pnt]
1.42857
0


[newcurve]
antrieb_wandler_lowrpmsoftness

[pnt]
0
0.4

[pnt]
1000
1



[newcurve]
retarder_fadein

[pnt]
0
0.5

[pnt]
0.4
1.5

[pnt]
0.6
1


[newcurve]
retarder_brakin_fadein

[pnt]
0
50

[pnt]
0.1
100

[pnt]
0.4
250

[pnt]
0.6
1

[const]
gear_efficiency
0.95

[const]
hybrid_performance_setting
2

'Actuator rate in 1/n per second (total range 0..1)

[const]
kickdown_stellglied_inc_rate
2

[const]
kickdown_stellglied_dec_rate
1

[const]
throttle_stellglied_inc_rate
0.2

[const]
throttle_stellglied_dec_rate
1

'minimum acceleration for upshift (m/s^2)

[const]
min_upshift_acceleration
-0.2

[newcurve]
Electricmotorstraction

[pnt]
0
1000

[pnt]
1
0

[newcurve]
RPM

[pnt]
0
700

[pnt]
1
2000












[newcurve]
hybrid_performance_setting_low

[pnt]
-12
0

[pnt]
0
1.59728

[pnt]
32
0.784532 




[newcurve]
hybrid_performance_setting_med

[pnt]
-50
0.98

[pnt]
0
1.96133

[pnt]
32
0.98









[newcurve]
hybridhoposensor

[pnt]
0
0.07

[pnt]
0.15
0.05


[pnt]
0.5
0.025

[pnt]
0.85
0


[newcurve]
hybridhoposensor_rpm

[pnt]
0.25
1

[pnt]
0.55
0.5

[pnt]
0.75
0.1


[newcurve]
hybridhoposensor_throttle

[pnt]
0.25
1

[pnt]
0.675
0.75

[pnt]
1
0.1




[newcurve]
hybrid_performance_setting_high

[pnt]
-12
1.96133

[pnt]
-3
1.96133

[pnt]
0
1.96133





[newcurve]
Hyb_Permo_1

[pnt]
30
0.3


[pnt]
40
0.3


[pnt]
64
0.7


[newcurve]
Hyb_Permo_2

[pnt]
0
0.1

[pnt]
40
0.5

[pnt]
80
0.7

[newcurve]
Hyb_Permo_3


[pnt]
32
0.75

[pnt]
50
1

[newcurve]
traction_motor_M_maxThrottle

[pnt]
800
500

[pnt]
2600
150

[pnt]
3200
0



[newcurve]
traction_motor_M_minThrottle

[pnt]
0
0

[newcurve]
traction_motor_power_drain_tempature

[pnt]
0
1

[pnt]
35
0.50



###
First value represents the axle speed
Second value represents the traction motor RPM speed to calculate the correct ratio

###
[newcurve]
traction_motor_A


[pnt]
0
1000

[pnt]
300
3700

[pnt]
1294
0

[pnt]
50
0

[pnt]
2200
5000

[newcurve]
traction_motor_B

[pnt]
0
0

[pnt]
1294
4200

[pnt]
1500
4600

[pnt]
3000
0


###Calculates the gear Ratio for the traction motor 
###Traction motor RPM is for the first value, supplied torque is the second value, based on 150 KW unit.

[newcurve]
traction_torque

[pnt]
0
525

[pnt]
2200
525

[pnt]
4200
300

[pnt]
7000
200

[pnt]
10000
0

[newcurve]
traction_peak

[pnt]
0
2

[pnt]
20
1

