[const]
engine_J
3.2



[const]
engine_consumption_curve_available
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
speedgov
135


[const]
rpmgov_unload
2200

[const]
rpmgov
2232

[const]
turbochaged
2


[const]
engine_governed_idle_RPM
650

Amount of watts used up during idle

[const]
engine_power_idle
25124

[const]
engine_coldM
-300 

[const]
engine_braking_coeffient
0.74

[newcurve]
engine_n_throttle


[pnt]
0.6
1


[pnt]
1
1.2


[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
0
120


[pnt]
800
195


[pnt]
1200
185


[pnt]
1400
185


[pnt]
1800
205

[pnt]
2000
205

[newcurve]
engine_M_maxThrottle

[pnt]
300
600

[pnt]
600
700


[pnt]
800
848



[pnt]
1200
1038.5565497


[pnt]
2100
857.86

[pnt]
2200
0





[newcurve]
engine_M_minThrottle


[pnt]
700
-50

[pnt]
800
-106


[pnt]
1000
-176

[pnt]
2400
-278.51


[pnt]
3000
-304


[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
1




[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2


[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_fuel_value
11.8
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
92

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
1000

[const]
engine_Qrate_fan_factor
1.38

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000







[newcurve]
governor


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
0

[newcurve]
rpmgov_map

[pnt]
-50
1

[pnt]
0
0





Pressure Ratio starts at 1:1, so an second  value at 0 would yield a pressure ratio of 1:1 or 14.7 PSI Non Aspirate Pressure with 0 PSI turbocharge boost.

[newcurve]
turbo_exhaust_flow



[pnt]
140
0

[pnt]
200
4.2

[pnt]
300
10.7


[pnt]
400
20.52

[pnt]
650
26.46

[pnt]
800
44.1





[const]
engine_volumetric_efficiency
90

Value in mm
[const]
turbo_compressor_wheel_size
80


[const]
turbo_min_psi
-1


[const]
turbo_max_psi
24.7556607




number of liters the engine has (CID) this helps calculate the spool rate of the turbocharger

[const]
engine_CID
9




[newcurve]
idle_ctr

[pnt]
-50
1


[pnt]
50
0




[newcurve]
engine_alternator_load

[pnt]
0
0

[pnt]
850
8.5

[pnt]
3000
11.114




[newcurve]
engine_throttle_sensitivity

[pnt]
0
0


[pnt]
1
1

[const]
VGT_turbochager
0


