[const]
engine_J
2.0

[const]
engine_rpm_limsup
3200

[const]
speed_governor_sw
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_governed_idle_RPM
500

[const]
engine_power_idle
22710

[const]
engine_coldM
-300

[newcurve]
governor
[pnt]
-100.00
0.8

[pnt]
75.00
0.5

[pnt]
76.00
0

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
100

[pnt]
592
150

[pnt]
600
200

[pnt]
1000
400

[pnt]
1400
450

[pnt]
1900
498

[pnt]
2100
489

[pnt]
2300
378

[pnt]
2350
300

[pnt]
2800
300

[pnt]
2900
300

[pnt]
3000
0


[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
0

[pnt]
650
-100

[pnt]
1900
-300

[pnt]
2800
-350

[pnt]
3000
-390


[newcurve]
engine_M_minT1000

[pnt]
50
0

[pnt]
300
250

[pnt]
592
50

[pnt]
1000
0

[pnt]
1500
-200

[pnt]
2500
-250


[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
0.6

[pnt]
800
0.8

[pnt]
1200
0.6

[pnt]
1700
0.45

[pnt]
2300
0.2


[newcurve]
engine_efficiency_throttle

[pnt]
0
1.3

[pnt]
0.8
1

[pnt]
1
1.2


[const]
engine_fuel_value
27
12.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
86

[const]
luefterthermostat_cls
80

[const]
kuehlerthermostat_opn
93

[const]
kuehlerthermostat_cls
80

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
3.0

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000
