[newcurve]
cockpit_tacholinie

[pnt]
0
0
[pnt]
5
0
[pnt]
10
13.9
[pnt]
20
24.8
[pnt]
30
46.9
[pnt]
40
69.2
[pnt]
50
91.4
[pnt]
60
113.4
[pnt]
70
134.9
[pnt]
80
156.5
[pnt]
90
178.4
[pnt]
100
200.9
[pnt]
110
223.1
[pnt]
120
245

[newcurve]
cockpit_battery_voltage_line

[pnt]
0
0

[pnt]
0.74
26

[pnt]
0.888
40

[pnt]
0.9629
47

[pnt]
1.037
55

[pnt]
1.11
68

[pnt]
1.19
90

[newcurve]
cockpit_revlinie

[pnt]
0
0
[pnt]
290
0
[pnt]
300
21
[pnt]
500
35
[pnt]
1000
80
[pnt]
1500
125
[pnt]
2000
170
[pnt]
2500
215
[pnt]
3000
248

[newcurve]
cockpit_oeldruck

[pnt]
300
0

[pnt]
400
1.1

[pnt]
1700
4.5

[newcurve]
odometer_10er-uebertrag
[pnt]
0
0
[pnt]
0.9
0
[pnt]
1
1

[newcurve]
cockpit_engine_temperature

[pnt]
0
0

[pnt]
60
17

[pnt]
80
31

[pnt]
90
45

[pnt]
100
58

[pnt]
110
68

[const]
automatic_battery_switch
1

[const]
auxheat_via_button
1

[const]
wiper_lever
0

[newcurve]
cockpit_warndruck

[pnt]
550000
1

[pnt]
700000
0

[const]
cockpit_gangwahltaster_alt
0

[const]
cockpit_zentralschmierung_dist
50

[const]
cockpit_zentralschmierung_maxtime
30

[const]
cockpit_gear_D_only
0

[const]
cockpit_has_20h_switch
0

[const]
cockpit_has_retarderswitch
1

[const]
cockpit_has_coolingswitch
1

[const]
cp_fahrertuer_anschlagseite
1

[const]
HH_funkpiep_active
0

[const]
cockpit_beep_time_sec
60


=============================================
Inverse Widerstände (Leitwerte) in 1/Ohm.


Allgemeiner Stromverbrauch Panel (sonstige): 1x40W (1x0.0174 1/Ohm)

[const]
cp_general_Rinv
0.0174

.............................

Frontheizgerät: 1x60W (1x0.104 1/Ohm)

[const]
cp_klimator_Rinv
0.104

.............................

Hintere Heizgeräte (zusammen): 60W (0.104 1/Ohm)

[const]
cp_cabinheater_Rinv
0.104
