
	[friendlyname]
VF Bus
VF 18
1

[sound]
Sound\sound_18.cfg

[sound_ai]
Sound\sound_18.cfg

[model]
model\model_18_Trail.cfg

[scriptshare]

[paths]
model\paths_18_Trail.cfg

[passengercabin]
model\passengercabin_18_Trai.cfg

	////////////////////////////////////////////////////////
		Scripts
	////////////////////////////////////////////////////////

[varnamelist]
26
script\AI_varlist.txt
script\Collision_varlist.txt
script\antrieb_varlist.txt
script\engine_turbo_varlist.txt
script\elec_varlist_turbo.txt
Script\bremse_varlist.txt
script\auspuff_varlist.txt
Script\lights_varlist.txt
Script\door_varlist.txt
script\wiper_varlist.txt
Script\cockpit_varlist.txt
script\klappern_varlist.txt
script\heizung_varlist.txt
script\rain_varlist.txt
script\dirt_varlist.txt
script\ticketprinter_varlist.txt
script\churakrueger\VMatrix_varlist.txt
script\wimpel_varlist.txt
script\visual_varlist.txt
script\cashdesk_varlist.txt
Script\VDV_varlist.txt
script\spray_varlist.txt
script\articulation_varlist.txt
script\IBIS_varlist.txt
script\Hybrid_Serial_Varlist.txt
script\ablak_varlist.txt

[stringvarnamelist]
5
script\ticketprinter_stringvarlist.txt
script\churakrueger\vMatrix_stringvarlist.txt
Script\cockpit_stringvarlist.txt
Script\VDV_stringvarlist.txt
script\IBIS_stringvarlist.txt


	////////////////////////////////////////////////////////
		Kameras *NEU01*
	////////////////////////////////////////////////////////


	0: Blick nach vorne (std)
[add_camera_driver]
0
4.68
1.84
-0.06
45
0
-10



################
Passagiersichten
################

	0: Blick nach vorne (std)
[add_camera_driver]
0
4.68
1.84
-0.06
45
0
-10


################
Passagiersichten
################

	0: Hinten links sitzend
[add_camera_pax]
-0.99
-1.925
2
-0.06
45
25
0

	1: Stehplatz an der Hintertuer
[add_camera_pax]
0
1
2.05
-0.06
45
90
0

	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	2: hinten rechts sitzend
[add_camera_pax]
0.08
-3.388
2.1
-0.06
45
-20
0

	Folgender Befehl setzt die Standardfahrerkamera:

[set_camera_std]
3

	Folgender Befehl setzt den Zentrierpunkt der AuЯenkamera:

[set_camera_outside_center]
0
0
1.2




	////////////////////////////////////////////////////////
		Physikalische und geometrische Grunddaten
	////////////////////////////////////////////////////////

[mass]
8.7

[momentofintertia]
118.6
31.6
118.6

[boundingbox]
2.52
7.5
2.4
0
-0.1
1.8

[cog]
0
0
0.8

[schwerpunkt]
0.9

[rollwiderstand]
580

[rot_pnt_long]
-0.4

[ai_deltaheight]
-0.10


	Hinterachse:

[newachse]
achse_long
-0.355
achse_maxwidth
2.42
achse_minwidth
1.2
achse_raddurchmesser
0.94
achse_feder
711.2
achse_maxforce
101.6
achse_daempfer
44.4
achse_antrieb
1

[coupling_front]
0
4.01738
0.4257

[couple_front_open_for_sound]

[coupling_front_character]
60
-20
20
1