[const]
engine_J
3.7

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
speedgov
72

[const]
rpmgov
2200

[const]
engine_governed_idle_RPM
700

[const]
engine_power_idle
22710

[const]
engine_coldM
-300



[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
592
300

[pnt]
900
930

[pnt]
1000
1025

[pnt]
1100
1047

[pnt]
1200
1050

[pnt]
1300
1050

[pnt]
1400
1045

[pnt]
1500
1020

[pnt]
1600
1000

[pnt]
1700
982

[pnt]
1800
942

[pnt]
1900
900

[pnt]
2000
875

[pnt]
2100
828

[pnt]
2200
800

[pnt]
2800
0



[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
592
50

[pnt]
700
0

[pnt]
1000
-150

[pnt]
2900
-250

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
1

[newcurve]
engine_efficiency_throttle

[pnt]
0
0.3

[pnt]
1
1
[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_consumption_curve_available
1
[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
0
120


[pnt]
800
238


[pnt]
900
222


[pnt]
1000
210


[pnt]
1100
204

[pnt]
1200
202

[pnt]
1300
186

[pnt]
1400
182

[pnt]
1500
182

[pnt]
1600
182

[pnt]
1700
183

[pnt]
1800
185

[pnt]
1900
188

[pnt]
2000
189

[pnt]
2100
202

[pnt]
2200
215

[pnt]
2300
220

[const]
engine_fuel_value
11.8
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000


First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.67


[pnt]
30
1



[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0

[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency


[pnt]
550
0.5

[pnt]
1000
1.00


[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
0

[pnt]
750
30


[newcurve]
turbo_inertia

[pnt]
0
3

[pnt]
10
30

[pnt]
30
90

[newcurve]
turbo_inertia_dec

[pnt]
0
0.5


[pnt]
30
30

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0


[pnt]
1
1


[newcurve]
governor
[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
-0.01




[newcurve]
rpmgov_map

[pnt]
-25
1

[pnt]
0
0




[newcurve]
engine_airflow

[pnt]
0
1


[pnt]
10
2

[const]
engine_init_time
4

[const]
engine_ignition_time
1

[newcurve]
engine_turbo_RPM_factor

[pnt]
0
0

[pnt]
800
0.5

[pnt]
1500
0.7

[pnt]
1800
0.9

[pnt]
2000
1


[newcurve]
engine_turbo_throttle_factor

[pnt]
0
0.5

[pnt]
1
1

[newcurve]
engine_turbo_boost

[pnt]
0
1

[pnt]
70
1

[pnt]
90
1

[pnt]
100
1

[const]
engine_coldM
-300

[newcurve]
engine_n_coldM

[pnt]
0
-140

[pnt]
2500
-350


[const]
engine_oelvis_M_nulldeg
-20

[const]
engine_oelvis_M_expfactor
-0.05