[const]
antrieb_kuppl_M_max
300

[const]
antrieb_kuppl_M_min
200

[const]
antrieb_getr_ratioR
-7.82

[const]
antrieb_getr_ratio1
6.4

[const]
antrieb_getr_ratio2
3.09

[const]
antrieb_getr_ratio3
1.69

[const]
antrieb_getr_ratio4
1.0

[const]
antrieb_i_achse
7.12

[const]
gear_engagement_tolerance
55

Propeller shaft rpm when gear shifts can take place (only for automatic gearbox and AI buses)

[const]
antrieb_getr_autoSwUpMinSpd1
360

[const]
antrieb_getr_autoSwUpMaxSpd1
380

[const]
antrieb_getr_autoSwDnMinSpd2
80

[const]
antrieb_getr_autoSwDnMaxSpd2
100

[const]
antrieb_getr_autoSwDnkickdnSpd2
480

[const]
antrieb_getr_autoSwDnAISpd2
350

[const]
antrieb_getr_autoSwUpMinSpd2
640

[const]
antrieb_getr_autoSwUpMaxSpd2
660

[const]
antrieb_getr_autoSwDnMinSpd3
470

[const]
antrieb_getr_autoSwDnMaxSpd3
495

[const]
antrieb_getr_autoSwDnkickdnSpd3
750

[const]
antrieb_getr_autoSwDnAISpd3
560

[const]
antrieb_getr_autoSwUpMinSpd3
980

[const]
antrieb_getr_autoSwUpMaxSpd3
1000

[const]
antrieb_getr_autoSwDnMinSpd4
900

[const]
antrieb_getr_autoSwDnMaxSpd4
920

[const]
antrieb_getr_autoSwDnkickdnSpd4
1160

[const]
antrieb_getr_autoSwDnAISpd4
900


[const]
antrieb_wandler_fillrate
1000


[const]
retarder_min_einschaltspeed
502

[const]
gear_efficiency
0.95

Defining the engine rpm

[newcurve]
engine_rpm_base

[pnt]
-5000
0

[pnt]
0
0

[pnt]
180
0

[pnt]
300
300

[pnt]
4000
4000

[pnt]
8000
6000

[newcurve]
engine_rpm_wandler_max

[pnt]
-5000
0

[pnt]
0
1000

[pnt]
180
850

[pnt]
300
600

[pnt]
500
450

[pnt]
1000
0

[pnt]
5000
0

[newcurve]
engine_rpm_wandler_min

[pnt]
-3000
0

[pnt]
0
500

[pnt]
180
500

[pnt]
300
200

[pnt]
500
0

[pnt]
1000
0

[newcurve]
engine_n_fluctuation

[pnt]
0
1

[pnt]
0.3
1.04

[pnt]
0.6
0.96

[pnt]
1.2
1.03

[pnt]
1.4
0.97

[pnt]
2
1.02

[pnt]
2.2
0.98

[pnt]
2.8
1.01

[pnt]
3
0.99

[pnt]
3.6
1.005

[pnt]
3.8
0.995

[pnt]
4
1

[const]
gear_efficiency_wandler
0.8

[const]
gear_efficiency_fest
0.95

Minimum acceleration for upshift (m/s^2)

[const]
min_upshift_acceleration
-0.2

[const]
centrifugal_clutch_engagement_start
250

[const]
centrifugal_clutch_engagement_full
1000

[newcurve]
centrifugal_clutch

[pnt]
0
0

[pnt]
250
0

[pnt]
1000
1