SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( 3356_1
	Type ( Engine )
	WagonShape ( 3356_1.s )
	Size  ( 3.006mm 3.728m 8.5m )
	CentreOfGravity ( 0m 1.7m 0m )
	Mass ( 35t )
	WheelRadius ( 0.359m )
	InertiaTensor ( Box (3.0m 3.7m 19.0m) )
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 2e7N/m 0  )
			Damping ( 0.2e7N/m/s 0 )
			Break ( 2e7N 0 )
			r0 ( 0.1 1e9 )
		)
		CouplingUniqueType( "Repas" )
		CouplingHasRigidConnection ()
	)
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 2e7N/m 0  )
			Damping ( 0.2e7N/m/s 0 )
			Break ( 2e7N 0 )
			r0 ( 0.1 1e9 )
		)
		CouplingUniqueType( "Repas" )
		CouplingHasRigidConnection ()
	)	
	Buffers (
		Spring (
			Stiffness ( 1e7N/m 0 )
			Damping ( 1e6N/m/s 0 )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 3cm )
	DerailRailForce ( 70kN )
	DerailBufferForce ( 40kN )
	NumWheels ( 4 )
	Friction (
		5N/m/s		1		1mph		1		1
		1.1N/rad/s		1		-1rad/s		1		1
	)
	
	AntiSlip ()

	BrakeEquipmentType( "EP_brake" )

	BrakeSystemType( "EP" )
	MaxBrakeForce( 60000N )

	EmergencyBrakeResMaxPressure( 50 )
	TripleValveRatio( 2.3 )
	MaxReleaseRate( 50 )
	MaxApplicationRate( 9 )
	MaxAuxilaryChargingRate( 4 )
	EmergencyResCapacity( 8 )
	EmergencyResChargingRate( 4 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )
	EmergencyResVolumeMultiplier( 1.15 )
	BrakeAirPressureGainInResForOnePoundFromPipe( 0.25 )

	BrakeDistributorFullServicePressure( 0 )
	BrakeDistributorMaxAuxilaryResPressure( 50 )
	BrakeDistributorEmergencyResPressure( 50 )
	BrakeDistributorReleaseRate( 10 )
	BrakeDistributorApplicationRate( 15 )
	BrakeDistributorTrainPipeControlRatio( 2.03 )
	BrakeDistributorNormalFullReleasePressure( 70 )
	PassengerCapacity ( 115 )

	Lights	( 6	
		Light	(
			comment( svetlo leve cervene )
			Type( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -0.9 1.635 9.46 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)

		Light	(
			comment( svetlo prave cervene )
			Type( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 0.9 1.635 9.46 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.5 )
					Elevation ( 0.0 0.0 0.0 )
					)
				)
			)
		
		Light	(
			comment( dvere 1 )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.4 3.2 6.925 )
					Azimuth ( 90.0 90.0 90.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)
		
		Light	(
			comment( dvere 2 )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.4 3.2 2.27 )
					Azimuth ( 90.0 90.0 90.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)	
		
		Light	(
			comment( dvere 3 )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.4 3.2 -2.27 )
					Azimuth ( 90.0 90.0 90.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)
		
		Light	(
			comment( dvere 4 )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.4 3.2 -6.925 )
					Azimuth ( 90.0 90.0 90.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)	
	)
)

Engine ( 3356_1
	Wagon ( 3356_1 )
	Type ( Electric )
	MaxPower ( 200kW )
	MaxForce ( 200kN )						
	MaxContinuousForce ( 90kN )					
	MaxVelocity ( 90kmh )
	MaxCurrent ( 470A )
	WheelRadius ( 0.425m )
	Sanding ( 1mph )
	NumWheels ( 4 ) 

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )

	EngineBrakesControllerDirectControlExponent( 2 )


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )

	EngineBrakesControllerDirectControlExponent( 2 )


	BrakesEngineControllers( "Train, Dynamic, Blended" )
	DoesBrakeCutPower( 1 )
	BrakeCutsPowerAtBrakeCylinderPressure( 50 )				

	AirBrakesAirCompressorPowerRating( 4 )
	AirBrakesMainMinResAirPressure( 30 )
	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 1 )
	AirBrakesAirCompressorWattage( 19000 )
	AirBrakesCompressorRestartPressure( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.5 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )
	AirBrakesHasLowPressureTest ( 1 )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 10 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	EngineBrakesControllerEmergencyApplicationRate( 10 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 10 )
	EngineBrakesControllerFullServicePressureDrop( 28 )

	TrainBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 10 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 90 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 10 )
	TrainBrakesControllerFullServicePressureDrop( 28 )

	DynamicBrakesMinUsableSpeed( 1 )
	DynamicBrakesMaximumEffectiveSpeed( 25 )
	DynamicBrakesMaximumForce( 140kn )
	DynamicBrakesResistorCurrentLimit ( 1600 )
	DynamicBrakesCutInSpeed( 1 )
	DynamicBrakesMaxAirBrakePressure ( 150 )
	DynamicBrakesFadingSpeed( 50 )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 150 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 8 )
	DynamicBrakeHasAutoBailOff( 0 )

	DoesHornTriggerBell( 0 )

    	EmergencyStopMonitor(
    		MonitoringDeviceMonitorTimeLimit( 0 )
    		MonitoringDeviceAlarmTimeLimit( 0 )
    		MonitoringDevicePenaltyTimeLimit( 0 )
    		MonitoringDeviceCriticalLevel( 0 )
    		MonitoringDeviceResetLevel( 0 )
    		MonitoringDeviceAppliesFullBrake( 1 )
    		MonitoringDeviceAppliesEmergencyBrake( 1 )
    		MonitoringDeviceAppliesCutsPower( 1 )
    		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed( 0 )
		MonitoringDeviceResetOnResetButton( 1 )
    		)
		
	VigilanceMonitor(
		MonitoringDeviceMonitorTimeLimit( 25 )
		MonitoringDeviceAlarmTimeLimit( 17 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 0 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		)

	OverspeedMonitor(
		MonitoringDeviceMonitorTimeLimit( 0 )
		MonitoringDeviceAlarmTimeLimit( 5 )
		MonitoringDevicePenaltyTimeLimit( 0 )
		MonitoringDeviceCriticalLevel( 106 )
		MonitoringDeviceResetLevel( 0 )
		MonitoringDeviceAppliesFullBrake( 1 )
		MonitoringDeviceAppliesEmergencyBrake( 1 )
		MonitoringDeviceAppliesCutsPower( 1 )
		MonitoringDeviceAppliesShutsDownEngine( 1 )
		MonitoringDeviceTriggerOnTrackOverspeed( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin( 2 )
		MonitoringDeviceResetOnZeroSpeed( 1 )
		MonitoringDeviceResetOnResetButton( 0 )
		MonitoringDeviceDoesSuppressionReset( 0 )
		)
	
        EngineControllers (
            Throttle ( 0 1 0.1 0 
                NumNotches ( 11 
                	Notch ( 0.0       0 Dummy )
			Notch ( 0.1       0 Dummy )
			Notch ( 0.2       0 Dummy )
			Notch ( 0.3       0 Dummy )
			Notch ( 0.4       0 Dummy )
			Notch ( 0.5       0 Dummy )
			Notch ( 0.6       0 Dummy )
			Notch ( 0.7       0 Dummy )
			Notch ( 0.8       0 Dummy )
			Notch ( 0.9       0 Dummy )
			Notch ( 1.0       0 Dummy )
                )	
            )
            Brake_Train ( 0 1 0.1 0.7
                NumNotches ( 3
                    Notch( 0   0 TrainBrakesControllerReleaseStart )
                    Notch( 0.2 1 TrainBrakesControllerEPApplyStart )
                    Notch( 0.8 0 TrainBrakesControllerEmergencyStart )
                )
            )

            DirControl ( -1 0 1 1 )
            Combined_Control( 0 1 0.5 0.75 throttle train )
            EmergencyStopToggle( 0 1 0 )
            AWS ( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Vigilance ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
            Wipers ( 0 1 0 )
            BellToggle( 0 1 0 )
            BailOffButton( 0 1 0 )
        )
    Name ( "3356_1" )
    Description (
	"8171M - Repas"
	)
	EngineOperatingProcedures (
	"To move forward\n"+
	"1.	Press the W key to move the Reverser to Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the D key to move the throttle from Idle to Notch 1.\n"+  
	"4.	Gradually increase power (D key), one notch at a time, until your train reaches the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+   
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+ 
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"4.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"5.	Slowly advance the throttle lever (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the 'permission to depart' signal.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 4 Km/h.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
	)