[const]
engine_J
2

[const]
engine_consumption_curve_available
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
1

[const]
engine_ASR
1

[const]
speedgov
107


[const]
rpmgov
2260

[const]
engine_governed_idle_RPM
650

[const]
engine_power_idle
25124

[const]
engine_coldM
-300

[newcurve]
engine_consumption_per_rpm

[pnt]
0
0

[pnt]
0
120


[pnt]
800
195


[pnt]
1100
190


[pnt]
1900
211


[pnt]
2800
255

[pnt]
4800
415

[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
540

[pnt]
600
1000

[pnt]
800
1030

[pnt]
1000
1050

[pnt]
1400
1050

[pnt]
1600
1025

[pnt]
1900
960

[pnt]
2300
750

[pnt]
2500
0




[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
350
350

[pnt]
592
0

[pnt]
650
-50

[pnt]
1000
-127

[pnt]
2500
-127
[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
600
1




[newcurve]
engine_efficiency_throttle

[pnt]
0
0.3

[pnt]
1
1

[newcurve]
engine_braking

[pnt]
0
1

[pnt]
1
0

[const]
engine_fuel_value
11.8
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250



[const]
luefterthermostat_opn
90

[const]
luefterthermostat_cls
87

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
82

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
300

[const]
engine_Qrate_fan_factor
1.15

[const]
engine_Qrate_veloc_factor_basic
200

[const]
engine_Qrate_veloc_factor
4

[const]
engine_cvm_engine
600000

[const]
engine_cvm_envir
10000



First is turbocharger PSI
Second is the torque mutipler
[newcurve]
turbo_M_max

[pnt]
0
0.55


[pnt]
30
1



[newcurve]
turbo_limit_thorttle_1

[pnt]
0
0


[pnt]
1
30

Controls the turbo boost using the engine rpm 
[newcurve]
turbo_engine_rpm_efficiency
[pnt]
0
0

[pnt]
700
0

[pnt]
850
0.3

[pnt]
1300
0.94

[pnt]
2200
1.00


[newcurve]
turbo_engine_rpm_max_psi
[pnt]
500
1

[pnt]
750
30


[newcurve]
turbo_inertia

[pnt]
0
1.5

[pnt]
5
3


[pnt]
10
13



[newcurve]
governor


[pnt]
0
1

[pnt]
1
0

[pnt]
1.01
-0.01

[newcurve]
rpmgov_map

[pnt]
-75
1

[pnt]
0
0

[newcurve]
turbo_inertia_dec

[pnt]
0
1


[pnt]
3
5

[pnt]
30
30

[newcurve]
turbo_M_inertia_throttle

[pnt]
0
0


[pnt]
1
1


[newcurve]
engine_airflow

[pnt]
0
1

[pnt]
20
2