[const]
engine_J
3.5

' Engine will automatically shutdown if RPM gets greater than this limit to prevent engine failure.

[const]
engine_rpm_limsup
2100

' Activates speed governor system (0 for disabled, 1 for enabled). Use curve
' Speed governor created by krtz07

[const]
speed_governor_sw
1

[const]
engine_speedcontrol
0

[const]
engine_e-gas
0

[const]
engine_ASR
0

[const]
engine_governed_idle_RPM
592

[const]
engine_power_idle
22710

[const]
engine_coldM
-300


############ SPEED LIMIT CURVE - by krtz07 ###########

[newcurve]
governor
[pnt]
-100.00
1

[pnt]
75.00
1

[pnt]
76.00
0

############ THROTTLE CURVE FOR MAX. INPUT ###########

[newcurve]
engine_M_maxThrottle_nom


[pnt]
50
0

[pnt]
300
400

[pnt]
592
500

[pnt]
600
510

[pnt]
1000
680

[pnt]
1400
890

[pnt]
1900
750

[pnt]
2100
721

[pnt]
2300
630

[pnt]
2350
0

############ THROTTLE CURVE FOR MIN. INPUT ###########

[newcurve]
engine_M_minThrottle_nom

[pnt]
50
0

[pnt]
300
250

[pnt]
550
0

[pnt]
650
-200

[pnt]
1900
-500

[pnt]
2800
-450

[pnt]
3000
-390


[newcurve]
engine_M_maxThrottle

[pnt]
50
0

[pnt]
300
400

[pnt]
592
500

[pnt]
600
510

[pnt]
1000
680

[pnt]
1400
890

[pnt]
1900
750

[pnt]
2100
721

[pnt]
2300
630

[pnt]
2350
0

[newcurve]
engine_M_minThrottle

[pnt]
50
0

[pnt]
300
250

[pnt]
550
0

[pnt]
650
-100

[pnt]
1000
-300

[pnt]
2500
-550

[newcurve]
engine_efficiency_rpm

[pnt]
0
0

[pnt]
800
1

[pnt]
1200
0.45

[pnt]
1700
0.45

[pnt]
2300
0.2

[newcurve]
engine_efficiency_throttle

[pnt]
0
0.3

[pnt]
1
1

	mértékegység: g/kWh
[newcurve]
engine_consumption_per_rpm

[pnt]
0
228

[pnt]
800
226

[pnt]
1000
225

[pnt]
1100
224

[pnt]
1300
224

[pnt]
1560
225

[pnt]
1800
228

[pnt]
2100
234

[pnt]
3100
259

[const]
engine_consumption_curve_available
1

[const]
engine_fuel_value
16
9.97
Heizwert Diesel: 11.8 kWh/kg mit Dichte 0.845 kg/l verrechnet

[const]
engine_tank_capacity
250


[const]
luefterthermostat_opn
92

[const]
luefterthermostat_cls
88

[const]
kuehlerthermostat_opn
85

[const]
kuehlerthermostat_cls
80

[newcurve]
kuehlwassersmoke

[pnt]
0
0

[pnt]
105
0

[pnt]
115
100


[const]
engine_Qrate_engine_factor
1.2

[const]
engine_Qrate_cooling_factor
700

[const]
engine_Qrate_fan_factor
0.9

[const]
engine_Qrate_veloc_factor_basic
1500

[const]
engine_Qrate_veloc_factor
100

[const]
engine_cvm_engine
362000

[const]
engine_cvm_envir
50000

[newcurve]
cockpit_tacho1

[pnt]
0
0

[pnt]
600
21

[pnt]
1400
110

[pnt]
3000
260